<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<library>
<packages>
<package name="DIP40">
</package>
<package name="DIP28-WIDE">
</package>
<package name="PLCC44-SOCKET">
</package>
<package name="DIL28-3">
</package>
<package name="ZIF28-6-WIDE">
</package>
<package name="JMP-1X2">
</package>
<package name="ADA-TFT-240X230-22INCH">
</package>
<package name="PDA6502-LOGO">
</package>
<package name="JP2">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
<package name="DIL08S">
<description>&lt;b&gt;CRYSTAL RESONATOR&lt;/b&gt;</description>
</package>
<package name="DIL14S">
<description>&lt;b&gt;CRYSTAL RESONATOR&lt;/b&gt;</description>
</package>
<package name="2X20">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X20-BIG">
</package>
<package name="1X12">
</package>
<package name="1X12_NO_SILK_KIT">
</package>
</packages>
<symbols>
<symbol name="W65C02">
<pin name="A15" direction="out"/>
<pin name="A14" direction="out"/>
<pin name="A13" direction="out"/>
<pin name="A12" direction="out"/>
<pin name="A11" direction="out"/>
<pin name="A10" direction="out"/>
<pin name="A9" direction="out"/>
<pin name="A8" direction="out"/>
<pin name="A7" direction="out"/>
<pin name="A6" direction="out"/>
<pin name="A5" direction="out"/>
<pin name="A4" direction="out"/>
<pin name="A3" direction="out"/>
<pin name="A2" direction="out"/>
<pin name="A1" direction="out"/>
<pin name="A0" direction="out"/>
<pin name="D7"/>
<pin name="D6"/>
<pin name="D5"/>
<pin name="D4"/>
<pin name="D3"/>
<pin name="D2"/>
<pin name="D1"/>
<pin name="D0"/>
<pin name="PHI2O" direction="out"/>
<pin name="SOB" direction="in" function="dot"/>
<pin name="RESB" direction="in" function="dot"/>
<pin name="PHI1O" direction="out"/>
<pin name="PHI2" direction="in" function="clk"/>
<pin name="NMIB" direction="in" function="dot"/>
<pin name="IRQB" direction="in" function="dot"/>
<pin name="RDY" direction="in"/>
<pin name="SYNC" direction="out"/>
<pin name="RWB" direction="out"/>
<pin name="MLB" direction="out"/>
<pin name="BE" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="VSS" direction="pwr"/>
<pin name="VPB" direction="out"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="W65C22">
<pin name="CA2"/>
<pin name="CA1" direction="in"/>
<pin name="PA7"/>
<pin name="PA6"/>
<pin name="PA5"/>
<pin name="PA4"/>
<pin name="PA3"/>
<pin name="PA2"/>
<pin name="PA1"/>
<pin name="PA0"/>
<pin name="PB7"/>
<pin name="PB6"/>
<pin name="PB5"/>
<pin name="PB4"/>
<pin name="PB3"/>
<pin name="PB2"/>
<pin name="PB1"/>
<pin name="PB0"/>
<pin name="CB2"/>
<pin name="CB1" direction="in"/>
<pin name="CS2B" direction="in" function="dot"/>
<pin name="CS1" direction="in"/>
<pin name="RWB" direction="in"/>
<pin name="RS3" direction="in"/>
<pin name="RS2" direction="in"/>
<pin name="RS1" direction="in"/>
<pin name="RS0" direction="in"/>
<pin name="D7"/>
<pin name="D6"/>
<pin name="D5"/>
<pin name="D4"/>
<pin name="D3"/>
<pin name="D2"/>
<pin name="D1"/>
<pin name="D0"/>
<pin name="IRQB" direction="oc" function="dot"/>
<pin name="PHI2" direction="in" function="clk"/>
<pin name="RESB" direction="in" function="dot"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="61256">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="!WE" direction="in"/>
<pin name="!OE" direction="in"/>
<pin name="!CE" direction="in"/>
<pin name="I/O0"/>
<pin name="I/O1"/>
<pin name="I/O2"/>
<pin name="I/O3"/>
<pin name="I/O4"/>
<pin name="I/O5"/>
<pin name="I/O6"/>
<pin name="I/O7"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="28C64">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="!WE" direction="in"/>
<pin name="!CE" direction="in"/>
<pin name="!OE" direction="in"/>
<pin name="D0" direction="hiz"/>
<pin name="D1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="D4" direction="hiz"/>
<pin name="D5" direction="hiz"/>
<pin name="D6" direction="hiz"/>
<pin name="D7" direction="hiz"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="NC@2" direction="nc"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="NC@1" direction="nc"/>
</symbol>
<symbol name="28C256">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="!WE" direction="in"/>
<pin name="!CE" direction="in"/>
<pin name="!OE" direction="in"/>
<pin name="D0" direction="hiz"/>
<pin name="D1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="D4" direction="hiz"/>
<pin name="D5" direction="hiz"/>
<pin name="D6" direction="hiz"/>
<pin name="D7" direction="hiz"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
</symbol>
<symbol name="JMP-1X2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="JP3E">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="QG3">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="TS" direction="pas"/>
</symbol>
<symbol name="PINH2X20">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="17" direction="pas" function="dot"/>
<pin name="18" direction="pas" function="dot"/>
<pin name="19" direction="pas" function="dot"/>
<pin name="20" direction="pas" function="dot"/>
<pin name="21" direction="pas" function="dot"/>
<pin name="22" direction="pas" function="dot"/>
<pin name="23" direction="pas" function="dot"/>
<pin name="24" direction="pas" function="dot"/>
<pin name="25" direction="pas" function="dot"/>
<pin name="26" direction="pas" function="dot"/>
<pin name="27" direction="pas" function="dot"/>
<pin name="28" direction="pas" function="dot"/>
<pin name="29" direction="pas" function="dot"/>
<pin name="30" direction="pas" function="dot"/>
<pin name="31" direction="pas" function="dot"/>
<pin name="32" direction="pas" function="dot"/>
<pin name="33" direction="pas" function="dot"/>
<pin name="34" direction="pas" function="dot"/>
<pin name="35" direction="pas" function="dot"/>
<pin name="36" direction="pas" function="dot"/>
<pin name="37" direction="pas" function="dot"/>
<pin name="38" direction="pas" function="dot"/>
<pin name="39" direction="pas" function="dot"/>
<pin name="40" direction="pas" function="dot"/>
</symbol>
<symbol name="M12">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="W65C02" prefix="U" uservalue="yes">
<description>8-bit microprocessor based on MOS 6502.</description>
<gates>
<gate name="G$1" symbol="W65C02"/>
</gates>
<devices>
<device name="DIP40" package="DIP40">
<connects>
<connect gate="G$1" pin="A0" pad="9"/>
<connect gate="G$1" pin="A1" pad="10"/>
<connect gate="G$1" pin="A10" pad="19"/>
<connect gate="G$1" pin="A11" pad="20"/>
<connect gate="G$1" pin="A12" pad="22"/>
<connect gate="G$1" pin="A13" pad="23"/>
<connect gate="G$1" pin="A14" pad="24"/>
<connect gate="G$1" pin="A15" pad="25"/>
<connect gate="G$1" pin="A2" pad="11"/>
<connect gate="G$1" pin="A3" pad="12"/>
<connect gate="G$1" pin="A4" pad="13"/>
<connect gate="G$1" pin="A5" pad="14"/>
<connect gate="G$1" pin="A6" pad="15"/>
<connect gate="G$1" pin="A7" pad="16"/>
<connect gate="G$1" pin="A8" pad="17"/>
<connect gate="G$1" pin="A9" pad="18"/>
<connect gate="G$1" pin="BE" pad="36"/>
<connect gate="G$1" pin="D0" pad="33"/>
<connect gate="G$1" pin="D1" pad="32"/>
<connect gate="G$1" pin="D2" pad="31"/>
<connect gate="G$1" pin="D3" pad="30"/>
<connect gate="G$1" pin="D4" pad="29"/>
<connect gate="G$1" pin="D5" pad="28"/>
<connect gate="G$1" pin="D6" pad="27"/>
<connect gate="G$1" pin="D7" pad="26"/>
<connect gate="G$1" pin="IRQB" pad="4"/>
<connect gate="G$1" pin="MLB" pad="5"/>
<connect gate="G$1" pin="NC" pad="35"/>
<connect gate="G$1" pin="NMIB" pad="6"/>
<connect gate="G$1" pin="PHI1O" pad="3"/>
<connect gate="G$1" pin="PHI2" pad="37"/>
<connect gate="G$1" pin="PHI2O" pad="39"/>
<connect gate="G$1" pin="RDY" pad="2"/>
<connect gate="G$1" pin="RESB" pad="40"/>
<connect gate="G$1" pin="RWB" pad="34"/>
<connect gate="G$1" pin="SOB" pad="38"/>
<connect gate="G$1" pin="SYNC" pad="7"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VPB" pad="1"/>
<connect gate="G$1" pin="VSS" pad="21"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PLCC44" package="PLCC44-SOCKET">
<connects>
<connect gate="G$1" pin="A0" pad="10"/>
<connect gate="G$1" pin="A1" pad="11"/>
<connect gate="G$1" pin="A10" pad="21"/>
<connect gate="G$1" pin="A11" pad="22"/>
<connect gate="G$1" pin="A12" pad="25"/>
<connect gate="G$1" pin="A13" pad="26"/>
<connect gate="G$1" pin="A14" pad="27"/>
<connect gate="G$1" pin="A15" pad="28"/>
<connect gate="G$1" pin="A2" pad="13"/>
<connect gate="G$1" pin="A3" pad="14"/>
<connect gate="G$1" pin="A4" pad="15"/>
<connect gate="G$1" pin="A5" pad="16"/>
<connect gate="G$1" pin="A6" pad="17"/>
<connect gate="G$1" pin="A7" pad="18"/>
<connect gate="G$1" pin="A8" pad="19"/>
<connect gate="G$1" pin="A9" pad="20"/>
<connect gate="G$1" pin="BE" pad="40"/>
<connect gate="G$1" pin="D0" pad="36"/>
<connect gate="G$1" pin="D1" pad="35"/>
<connect gate="G$1" pin="D2" pad="34"/>
<connect gate="G$1" pin="D3" pad="33"/>
<connect gate="G$1" pin="D4" pad="32"/>
<connect gate="G$1" pin="D5" pad="31"/>
<connect gate="G$1" pin="D6" pad="30"/>
<connect gate="G$1" pin="D7" pad="29"/>
<connect gate="G$1" pin="IRQB" pad="5"/>
<connect gate="G$1" pin="MLB" pad="6"/>
<connect gate="G$1" pin="NC" pad="12 39"/>
<connect gate="G$1" pin="NMIB" pad="7"/>
<connect gate="G$1" pin="PHI1O" pad="4"/>
<connect gate="G$1" pin="PHI2" pad="41"/>
<connect gate="G$1" pin="PHI2O" pad="43"/>
<connect gate="G$1" pin="RDY" pad="3"/>
<connect gate="G$1" pin="RESB" pad="44"/>
<connect gate="G$1" pin="RWB" pad="38"/>
<connect gate="G$1" pin="SOB" pad="42"/>
<connect gate="G$1" pin="SYNC" pad="8"/>
<connect gate="G$1" pin="VDD" pad="9 37"/>
<connect gate="G$1" pin="VPB" pad="2"/>
<connect gate="G$1" pin="VSS" pad="1 23 24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="W65C22" prefix="U" uservalue="yes">
<description>The W65C22 (W65C22N and W65C22S) Versatile Interface Adapter (VIA) is a
flexible I/O device for use with the 65xx series microprocessor family. The
W65C22 includes functions for programmed control of two peripheral ports (Ports
A and B). Two program controlled 8-bit bidirectional peripheral I/O ports allow
direct interfacing between the microprocessor and selected peripheral units.
Each port has input data latching capability. Two programmable Data Direction
Registers (A and B) allow selection of data direction (input or output) on an
individual line basis. Also provided are two programmable 16-bit Interval
Timer/Counters with latches. Timer 1 may be operated in a One-Shot Interrupt
Mode with interrupts on each count to zero, or in a Free-Run Mode with a
continuous series of evenly spaced interrupts. Timer 2 functions as both an
interval and pulse counter. Serial Data transfers are provided by a serial to
parallel/parallel to serial shift register. Application versatility is further
increased by various control registers, including an Interrupt Flag Register,
an Interrupt Enable Register and two Function Control Registers.</description>
<gates>
<gate name="G$1" symbol="W65C22"/>
</gates>
<devices>
<device name="DIP40" package="DIP40">
<connects>
<connect gate="G$1" pin="CA1" pad="40"/>
<connect gate="G$1" pin="CA2" pad="39"/>
<connect gate="G$1" pin="CB1" pad="18"/>
<connect gate="G$1" pin="CB2" pad="19"/>
<connect gate="G$1" pin="CS1" pad="24"/>
<connect gate="G$1" pin="CS2B" pad="23"/>
<connect gate="G$1" pin="D0" pad="33"/>
<connect gate="G$1" pin="D1" pad="32"/>
<connect gate="G$1" pin="D2" pad="31"/>
<connect gate="G$1" pin="D3" pad="30"/>
<connect gate="G$1" pin="D4" pad="29"/>
<connect gate="G$1" pin="D5" pad="28"/>
<connect gate="G$1" pin="D6" pad="27"/>
<connect gate="G$1" pin="D7" pad="26"/>
<connect gate="G$1" pin="IRQB" pad="21"/>
<connect gate="G$1" pin="PA0" pad="2"/>
<connect gate="G$1" pin="PA1" pad="3"/>
<connect gate="G$1" pin="PA2" pad="4"/>
<connect gate="G$1" pin="PA3" pad="5"/>
<connect gate="G$1" pin="PA4" pad="6"/>
<connect gate="G$1" pin="PA5" pad="7"/>
<connect gate="G$1" pin="PA6" pad="8"/>
<connect gate="G$1" pin="PA7" pad="9"/>
<connect gate="G$1" pin="PB0" pad="10"/>
<connect gate="G$1" pin="PB1" pad="11"/>
<connect gate="G$1" pin="PB2" pad="12"/>
<connect gate="G$1" pin="PB3" pad="13"/>
<connect gate="G$1" pin="PB4" pad="14"/>
<connect gate="G$1" pin="PB5" pad="15"/>
<connect gate="G$1" pin="PB6" pad="16"/>
<connect gate="G$1" pin="PB7" pad="17"/>
<connect gate="G$1" pin="PHI2" pad="25"/>
<connect gate="G$1" pin="RESB" pad="34"/>
<connect gate="G$1" pin="RS0" pad="38"/>
<connect gate="G$1" pin="RS1" pad="37"/>
<connect gate="G$1" pin="RS2" pad="36"/>
<connect gate="G$1" pin="RS3" pad="35"/>
<connect gate="G$1" pin="RWB" pad="22"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PLCC44-SOCKET" package="PLCC44-SOCKET">
<connects>
<connect gate="G$1" pin="CA1" pad="44"/>
<connect gate="G$1" pin="CA2" pad="43"/>
<connect gate="G$1" pin="CB1" pad="19"/>
<connect gate="G$1" pin="CB2" pad="20"/>
<connect gate="G$1" pin="CS1" pad="26"/>
<connect gate="G$1" pin="CS2B" pad="25"/>
<connect gate="G$1" pin="D0" pad="36"/>
<connect gate="G$1" pin="D1" pad="35"/>
<connect gate="G$1" pin="D2" pad="34"/>
<connect gate="G$1" pin="D3" pad="32"/>
<connect gate="G$1" pin="D4" pad="31"/>
<connect gate="G$1" pin="D5" pad="30"/>
<connect gate="G$1" pin="D6" pad="29"/>
<connect gate="G$1" pin="D7" pad="28"/>
<connect gate="G$1" pin="IRQB" pad="23"/>
<connect gate="G$1" pin="PA0" pad="2"/>
<connect gate="G$1" pin="PA1" pad="3"/>
<connect gate="G$1" pin="PA2" pad="4"/>
<connect gate="G$1" pin="PA3" pad="5"/>
<connect gate="G$1" pin="PA4" pad="6"/>
<connect gate="G$1" pin="PA5" pad="7"/>
<connect gate="G$1" pin="PA6" pad="8"/>
<connect gate="G$1" pin="PA7" pad="9"/>
<connect gate="G$1" pin="PB0" pad="10"/>
<connect gate="G$1" pin="PB1" pad="12"/>
<connect gate="G$1" pin="PB2" pad="13"/>
<connect gate="G$1" pin="PB3" pad="14"/>
<connect gate="G$1" pin="PB4" pad="15"/>
<connect gate="G$1" pin="PB5" pad="16"/>
<connect gate="G$1" pin="PB6" pad="17"/>
<connect gate="G$1" pin="PB7" pad="18"/>
<connect gate="G$1" pin="PHI2" pad="27"/>
<connect gate="G$1" pin="RESB" pad="37"/>
<connect gate="G$1" pin="RS0" pad="42"/>
<connect gate="G$1" pin="RS1" pad="41"/>
<connect gate="G$1" pin="RS2" pad="40"/>
<connect gate="G$1" pin="RS3" pad="39"/>
<connect gate="G$1" pin="RWB" pad="24"/>
<connect gate="G$1" pin="VDD" pad="21"/>
<connect gate="G$1" pin="VSS" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UM61256AK-12" prefix="U" uservalue="yes">
<description>5V 32K x 8 CMOS 12ns SRAM</description>
<gates>
<gate name="G$1" symbol="61256"/>
</gates>
<devices>
<device name="" package="DIL28-3">
<connects>
<connect gate="G$1" pin="!CE" pad="20"/>
<connect gate="G$1" pin="!OE" pad="22"/>
<connect gate="G$1" pin="!WE" pad="27"/>
<connect gate="G$1" pin="A0" pad="10"/>
<connect gate="G$1" pin="A1" pad="9"/>
<connect gate="G$1" pin="A10" pad="21"/>
<connect gate="G$1" pin="A11" pad="23"/>
<connect gate="G$1" pin="A12" pad="2"/>
<connect gate="G$1" pin="A13" pad="26"/>
<connect gate="G$1" pin="A14" pad="1"/>
<connect gate="G$1" pin="A2" pad="8"/>
<connect gate="G$1" pin="A3" pad="7"/>
<connect gate="G$1" pin="A4" pad="6"/>
<connect gate="G$1" pin="A5" pad="5"/>
<connect gate="G$1" pin="A6" pad="4"/>
<connect gate="G$1" pin="A7" pad="3"/>
<connect gate="G$1" pin="A8" pad="25"/>
<connect gate="G$1" pin="A9" pad="24"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="I/O0" pad="11"/>
<connect gate="G$1" pin="I/O1" pad="12"/>
<connect gate="G$1" pin="I/O2" pad="13"/>
<connect gate="G$1" pin="I/O3" pad="15"/>
<connect gate="G$1" pin="I/O4" pad="16"/>
<connect gate="G$1" pin="I/O5" pad="17"/>
<connect gate="G$1" pin="I/O6" pad="18"/>
<connect gate="G$1" pin="I/O7" pad="19"/>
<connect gate="G$1" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="28C64" prefix="U" uservalue="yes">
<description>5V 8K x 8 CMOS EEPROM</description>
<gates>
<gate name="G$1" symbol="28C64"/>
</gates>
<devices>
<device name="DIP28-6-WIDE" package="DIP28-WIDE">
<connects>
<connect gate="G$1" pin="!CE" pad="20"/>
<connect gate="G$1" pin="!OE" pad="22"/>
<connect gate="G$1" pin="!WE" pad="27"/>
<connect gate="G$1" pin="A0" pad="10"/>
<connect gate="G$1" pin="A1" pad="9"/>
<connect gate="G$1" pin="A10" pad="21"/>
<connect gate="G$1" pin="A11" pad="23"/>
<connect gate="G$1" pin="A12" pad="2"/>
<connect gate="G$1" pin="A2" pad="8"/>
<connect gate="G$1" pin="A3" pad="7"/>
<connect gate="G$1" pin="A4" pad="6"/>
<connect gate="G$1" pin="A5" pad="5"/>
<connect gate="G$1" pin="A6" pad="4"/>
<connect gate="G$1" pin="A7" pad="3"/>
<connect gate="G$1" pin="A8" pad="25"/>
<connect gate="G$1" pin="A9" pad="24"/>
<connect gate="G$1" pin="D0" pad="11"/>
<connect gate="G$1" pin="D1" pad="12"/>
<connect gate="G$1" pin="D2" pad="13"/>
<connect gate="G$1" pin="D3" pad="15"/>
<connect gate="G$1" pin="D4" pad="16"/>
<connect gate="G$1" pin="D5" pad="17"/>
<connect gate="G$1" pin="D6" pad="18"/>
<connect gate="G$1" pin="D7" pad="19"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="NC@1" pad="1"/>
<connect gate="G$1" pin="NC@2" pad="26"/>
<connect gate="G$1" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ZIF28-6-WIDE" package="ZIF28-6-WIDE">
<connects>
<connect gate="G$1" pin="!CE" pad="20"/>
<connect gate="G$1" pin="!OE" pad="22"/>
<connect gate="G$1" pin="!WE" pad="27"/>
<connect gate="G$1" pin="A0" pad="10"/>
<connect gate="G$1" pin="A1" pad="9"/>
<connect gate="G$1" pin="A10" pad="21"/>
<connect gate="G$1" pin="A11" pad="23"/>
<connect gate="G$1" pin="A12" pad="2"/>
<connect gate="G$1" pin="A2" pad="8"/>
<connect gate="G$1" pin="A3" pad="7"/>
<connect gate="G$1" pin="A4" pad="6"/>
<connect gate="G$1" pin="A5" pad="5"/>
<connect gate="G$1" pin="A6" pad="4"/>
<connect gate="G$1" pin="A7" pad="3"/>
<connect gate="G$1" pin="A8" pad="25"/>
<connect gate="G$1" pin="A9" pad="24"/>
<connect gate="G$1" pin="D0" pad="11"/>
<connect gate="G$1" pin="D1" pad="12"/>
<connect gate="G$1" pin="D2" pad="13"/>
<connect gate="G$1" pin="D3" pad="15"/>
<connect gate="G$1" pin="D4" pad="16"/>
<connect gate="G$1" pin="D5" pad="17"/>
<connect gate="G$1" pin="D6" pad="18"/>
<connect gate="G$1" pin="D7" pad="19"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="NC@1" pad="1"/>
<connect gate="G$1" pin="NC@2" pad="26"/>
<connect gate="G$1" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="28C256" prefix="U">
<gates>
<gate name="G$1" symbol="28C256"/>
</gates>
<devices>
<device name="-ZIF" package="ZIF28-6-WIDE">
<connects>
<connect gate="G$1" pin="!CE" pad="20"/>
<connect gate="G$1" pin="!OE" pad="22"/>
<connect gate="G$1" pin="!WE" pad="27"/>
<connect gate="G$1" pin="A0" pad="10"/>
<connect gate="G$1" pin="A1" pad="9"/>
<connect gate="G$1" pin="A10" pad="21"/>
<connect gate="G$1" pin="A11" pad="23"/>
<connect gate="G$1" pin="A12" pad="2"/>
<connect gate="G$1" pin="A13" pad="26"/>
<connect gate="G$1" pin="A14" pad="1"/>
<connect gate="G$1" pin="A2" pad="8"/>
<connect gate="G$1" pin="A3" pad="7"/>
<connect gate="G$1" pin="A4" pad="6"/>
<connect gate="G$1" pin="A5" pad="5"/>
<connect gate="G$1" pin="A6" pad="4"/>
<connect gate="G$1" pin="A7" pad="3"/>
<connect gate="G$1" pin="A8" pad="25"/>
<connect gate="G$1" pin="A9" pad="24"/>
<connect gate="G$1" pin="D0" pad="11"/>
<connect gate="G$1" pin="D1" pad="12"/>
<connect gate="G$1" pin="D2" pad="13"/>
<connect gate="G$1" pin="D3" pad="15"/>
<connect gate="G$1" pin="D4" pad="16"/>
<connect gate="G$1" pin="D5" pad="17"/>
<connect gate="G$1" pin="D6" pad="18"/>
<connect gate="G$1" pin="D7" pad="19"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JMP-1X2" prefix="JP" uservalue="yes">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="JMP-1X2"/>
</gates>
<devices>
<device name="TH" package="JMP-1X2">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JP2E" prefix="JP" uservalue="yes">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="JP3E"/>
</gates>
<devices>
<device name="" package="JP2">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XO-" prefix="QG" uservalue="yes">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="QG3"/>
</gates>
<devices>
<device name="8" package="DIL08S">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="OUT" pad="5"/>
<connect gate="G$1" pin="TS" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="14" package="DIL14S">
<connects>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="OUT" pad="8"/>
<connect gate="G$1" pin="TS" pad="1"/>
<connect gate="G$1" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X20" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X20"/>
</gates>
<devices>
<device name="" package="2X20">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="19" pad="19"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="20" pad="20"/>
<connect gate="A" pin="21" pad="21"/>
<connect gate="A" pin="22" pad="22"/>
<connect gate="A" pin="23" pad="23"/>
<connect gate="A" pin="24" pad="24"/>
<connect gate="A" pin="25" pad="25"/>
<connect gate="A" pin="26" pad="26"/>
<connect gate="A" pin="27" pad="27"/>
<connect gate="A" pin="28" pad="28"/>
<connect gate="A" pin="29" pad="29"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="30" pad="30"/>
<connect gate="A" pin="31" pad="31"/>
<connect gate="A" pin="32" pad="32"/>
<connect gate="A" pin="33" pad="33"/>
<connect gate="A" pin="34" pad="34"/>
<connect gate="A" pin="35" pad="35"/>
<connect gate="A" pin="36" pad="36"/>
<connect gate="A" pin="37" pad="37"/>
<connect gate="A" pin="38" pad="38"/>
<connect gate="A" pin="39" pad="39"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="40" pad="40"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-BIG" package="2X20-BIG">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="19" pad="19"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="20" pad="20"/>
<connect gate="A" pin="21" pad="21"/>
<connect gate="A" pin="22" pad="22"/>
<connect gate="A" pin="23" pad="23"/>
<connect gate="A" pin="24" pad="24"/>
<connect gate="A" pin="25" pad="25"/>
<connect gate="A" pin="26" pad="26"/>
<connect gate="A" pin="27" pad="27"/>
<connect gate="A" pin="28" pad="28"/>
<connect gate="A" pin="29" pad="29"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="30" pad="30"/>
<connect gate="A" pin="31" pad="31"/>
<connect gate="A" pin="32" pad="32"/>
<connect gate="A" pin="33" pad="33"/>
<connect gate="A" pin="34" pad="34"/>
<connect gate="A" pin="35" pad="35"/>
<connect gate="A" pin="36" pad="36"/>
<connect gate="A" pin="37" pad="37"/>
<connect gate="A" pin="38" pad="38"/>
<connect gate="A" pin="39" pad="39"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="40" pad="40"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M12" prefix="JP">
<description>&lt;b&gt;Header 12&lt;/b&gt;
Standard 12-pin 0.1" header. Use with straight break away headers (SKU : PRT-00116), right angle break away headers (PRT-00553), swiss pins (PRT-00743), machine pins (PRT-00117), and female headers (PRT-00115).</description>
<gates>
<gate name="G$1" symbol="M12"/>
</gates>
<devices>
<device name="PTH" package="1X12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1X12_NO_SILK_KIT" package="1X12_NO_SILK_KIT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>