(footprint "Jack_3.5mm_XKB_PJ-3270_Horizontal" (version 20210722) (generator pcbnew) (layer "F.Cu")
  (tedit 61157A8E)
  (descr "3.5 mm, Stereo, Right Angle, Surface Mount (SMT), Audio Jack Connector (https://datasheet.lcsc.com/lcsc/2002271813_XKB-Connectivity-PJ-3270_C381134.pdf)")
  (tags "3.5mm audio xkb horizontal jack stereo")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -3.5) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 9591bb4c-23b0-4614-94e9-eaf0adf35688)
  )
  (fp_text value "Jack_3.5mm_XKB_PJ-3270_Horizontal" (at 0 13.9) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 1cd624b5-f8db-4090-9a72-0217feb064d8)
  )
  (fp_text user "${REFERENCE}" (at 0 6) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 2c10ae2f-2d8f-4fc4-aa24-7b07a7324c62)
  )
  (fp_line (start 3.1 2.7) (end 3.1 4.3) (layer "F.SilkS") (width 0.12) (tstamp 1df314b1-7c15-4d36-8c25-c197bf2dd233))
  (fp_line (start -3.1 1.6) (end -3.1 0.1) (layer "F.SilkS") (width 0.12) (tstamp 2375ccee-dfd9-4f37-8cb3-b9f105365ec4))
  (fp_line (start -3.1 8.3) (end -3.1 3.6) (layer "F.SilkS") (width 0.12) (tstamp 4a30b50d-656f-4267-b01b-fff3708874a4))
  (fp_line (start -3.1 12.15) (end -3.1 10.3) (layer "F.SilkS") (width 0.12) (tstamp 4c68ae96-e85a-4e67-a08e-124fb2dd8d57))
  (fp_line (start 3.1 12.15) (end -3.1 12.15) (layer "F.SilkS") (width 0.12) (tstamp 97de1db5-6f18-41d5-89a3-5895f9562bcd))
  (fp_line (start 3.1 0.7) (end 3.1 0.1) (layer "F.SilkS") (width 0.12) (tstamp d27f49c8-25b4-4fc7-a5c2-b86173748aca))
  (fp_line (start 3.1 6.3) (end 3.1 12.15) (layer "F.SilkS") (width 0.12) (tstamp dd91d8c7-7d19-4f36-9aff-879746f41ea9))
  (fp_line (start 3.5 12.7) (end -3.5 12.7) (layer "F.CrtYd") (width 0.05) (tstamp 13982317-6155-4f6e-bf5e-97211eb1614d))
  (fp_line (start -3.5 -2.5) (end 3.5 -2.5) (layer "F.CrtYd") (width 0.05) (tstamp 45fe9c8d-3b50-4c9a-875e-731c90a5c5f4))
  (fp_line (start 3.5 -2.5) (end 3.5 12.7) (layer "F.CrtYd") (width 0.05) (tstamp 8140684f-7467-4c16-9637-ed52f9e1cf8c))
  (fp_line (start -3.5 12.7) (end -3.5 -2.5) (layer "F.CrtYd") (width 0.05) (tstamp 8cf8500d-e2b4-4bc9-ae21-8532b77704be))
  (fp_line (start -3 0) (end -2.5 0) (layer "F.Fab") (width 0.1) (tstamp 0a032c77-7c33-45cc-bcd2-08d28de27f31))
  (fp_line (start 2.5 0) (end 3 0) (layer "F.Fab") (width 0.1) (tstamp 0ded0fa9-a74c-4c8f-aa23-6aaee2a1b910))
  (fp_line (start -2.5 0) (end -2.5 -2) (layer "F.Fab") (width 0.1) (tstamp 0f13c0d6-986e-4829-8eb3-ecac3290c0b3))
  (fp_line (start -2.5 -2) (end 2.5 -2) (layer "F.Fab") (width 0.1) (tstamp 18ce8c43-f494-45f3-ade4-75883112096c))
  (fp_line (start 2.5 -2) (end 2.5 0) (layer "F.Fab") (width 0.1) (tstamp 2d5051a6-8aaa-4884-9512-066cd95636a1))
  (fp_line (start 3 12.05) (end -3 12.05) (layer "F.Fab") (width 0.1) (tstamp 44a21e25-f239-4e55-bcbe-a8434f978732))
  (fp_line (start 3 0) (end 3 12.05) (layer "F.Fab") (width 0.1) (tstamp 4f10c8c9-2aed-458d-bfde-bc8fe8c24091))
  (fp_line (start -3 12.05) (end -3 0) (layer "F.Fab") (width 0.1) (tstamp c3012e8e-62d1-47e4-bc66-9b604492c313))
  (pad "" np_thru_hole circle locked (at 0 9) (size 1.2 1.2) (drill 1.2) (layers F&B.Cu *.Mask) (tstamp 280e02a9-3cdc-42fb-b79c-27a96b04bf96))
  (pad "" np_thru_hole circle locked (at 0 3) (size 1.2 1.2) (drill 1.2) (layers F&B.Cu *.Mask) (tstamp 5eda6686-3c08-493f-8939-0b5ef5018d60))
  (pad "R1" thru_hole oval (at 2.42 5.3 90) (size 2 1.3) (drill oval 1.5 0.8) (layers *.Cu *.Mask) (tstamp 87676d02-9852-4ebb-81c1-57f2b360194c))
  (pad "R2" thru_hole oval (at 2.42 1.7 90) (size 2 1.3) (drill oval 1.5 0.8) (layers *.Cu *.Mask) (tstamp ec0a47ae-210f-4e91-af2f-76ea4b650293))
  (pad "S" thru_hole oval (at -2.42 2.6 90) (size 2 1.3) (drill oval 1.5 0.8) (layers *.Cu *.Mask) (tstamp db41f74e-b3b3-46e4-8680-b6ac54676255))
  (pad "T" thru_hole oval (at -2.42 9.3 90) (size 2 1.3) (drill oval 1.5 0.8) (layers *.Cu *.Mask) (tstamp d35d5c4e-0f64-42b4-936d-d1b999b9d534))
  (pad "TN" thru_hole oval (at 2.22 11 90) (size 2 1.3) (drill oval 1.5 0.8) (layers *.Cu *.Mask) (tstamp 2387fba8-e7ca-4016-9aac-72bba0f4d2d5))
  (model "${KIPRJMOD}/Amber.3dshapes/Jack_3.5mm_XKB_PJ-3270_Horizontal.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
