(footprint "DrillSlot_Plated_5x3mm" (version 20210228) (generator pcbnew) (layer "F.Cu")
  (tedit 608882D4)
  (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp e52ad8c7-a210-4717-b2d0-3ea424f7e6c1)
  )
  (fp_text value "DrillSlot_Plated_5x3mm" (at 0 1 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c8f02b4e-85d5-415b-8d15-7a8159e2be21)
  )
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp af8338d2-63c8-49c7-8f3f-eba4d7a7adc3)
  )
  (pad "" thru_hole oval (at 0 0) (size 5.3 3.3) (drill oval 5 3) (layers *.Cu *.Mask) (tstamp f9631126-7144-462d-97fa-3fe4a6d42d04))
)
