(footprint "L_CommonModeChoke_Pulse_T811x" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 6124CE97)
  (descr "Pulse T811x Series Common Mode Chokes/Fitlers")
  (tags "surface mount common mode choke")
  (fp_text reference "REF**" (at 0 -3.9 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 6e2d850e-ae31-4ab1-92e0-69f9ad228ffe)
  )
  (fp_text value "L_CommonModeChoke_Pulse_T811x" (at 0 5 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c84a6be0-e3d0-4613-82f1-584b6a13497e)
  )
  (fp_text user "${REFERENCE}" (at 0 3.6 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 1432a0cf-3d9e-4302-bd7c-5e706dca22c9)
  )
  (fp_line (start -4.7 -2.2) (end -4.7 -3.4) (layer "F.SilkS") (width 0.12) (tstamp 5ac64d93-0584-4eea-8973-77572d1cf092))
  (fp_line (start -4.7 -3.4) (end -3.5 -3.4) (layer "F.SilkS") (width 0.12) (tstamp f382fdcf-cb34-4fa6-92fa-a92c91d31564))
  (fp_rect (start -3.3 -3.2) (end 3.3 3.2) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 2d847872-2c1b-411f-b3e6-225796c42a8d))
  (fp_rect (start -4.6 -3.3) (end 4.6 3.3) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp 59f67454-dba3-4570-8737-dfd309d07590))
  (pad "1" smd roundrect (at -2.5 -1.25) (size 4 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 02582e87-7f36-451a-8fdc-5e003e7b03c7))
  (pad "2" smd roundrect (at -2.5 1.25) (size 4 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 9fb17bd7-6f17-4efb-a2e5-2c1c01abe4f2))
  (pad "3" smd roundrect (at 3 1.25) (size 3 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp f7ca433b-e2fe-4728-8c74-c4df259907b7))
  (pad "4" smd roundrect (at 3 -1.25) (size 3 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp c2203508-36eb-479c-b89c-28088d985aba))
  (model "${KIPRJMOD}/Yellow.3dshapes/L_CommonModeChoke_Murata_DLW5B.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
