(footprint "L_CommonModeChoke_Murata_DLW5B" (version 20210722) (generator pcbnew) (layer "F.Cu")
  (tedit 6124CE97)
  (descr "Murata DLW5B Series Common Mode Chokes/Fitlers")
  (tags "surface mount common mode choke")
  (fp_text reference "REF**" (at 0 -3.6 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 6e2d850e-ae31-4ab1-92e0-69f9ad228ffe)
  )
  (fp_text value "L_CommonModeChoke_Murata_DLW5B" (at 0 5 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c84a6be0-e3d0-4613-82f1-584b6a13497e)
  )
  (fp_text user "${REFERENCE}" (at 0 3.6 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 1432a0cf-3d9e-4302-bd7c-5e706dca22c9)
  )
  (fp_line (start -2.8 -1.6) (end -2.8 -2.8) (layer "F.SilkS") (width 0.12) (tstamp 5ac64d93-0584-4eea-8973-77572d1cf092))
  (fp_line (start -2.8 -2.8) (end -1.6 -2.8) (layer "F.SilkS") (width 0.12) (tstamp f382fdcf-cb34-4fa6-92fa-a92c91d31564))
  (fp_rect (start -2.6 -2.6) (end 2.6 2.6) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 2d847872-2c1b-411f-b3e6-225796c42a8d))
  (fp_rect (start -2.7 -2.7) (end 2.7 2.7) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp 59f67454-dba3-4570-8737-dfd309d07590))
  (fp_line (start 2.5 2.5) (end -2.5 2.5) (layer "F.Fab") (width 0.1) (tstamp 43080e57-3248-4eb1-9215-7f42b505e9bc))
  (fp_line (start -2.5 2.5) (end -2.5 -2) (layer "F.Fab") (width 0.1) (tstamp 92cedb1d-9aa3-4e89-8ba9-af082aef83a8))
  (fp_line (start -2 -2.5) (end 2.5 -2.5) (layer "F.Fab") (width 0.1) (tstamp 959cdf8e-87da-4871-bee5-dd11b8716ace))
  (fp_line (start 2.5 -2.5) (end 2.5 2.5) (layer "F.Fab") (width 0.1) (tstamp b9c93258-b77e-4548-9023-9006088783a7))
  (fp_line (start -2.5 -2) (end -2 -2.5) (layer "F.Fab") (width 0.1) (tstamp f2c3d12b-2aa3-4c9d-bade-66df696fbfca))
  (pad "1" smd roundrect (at -1.5 -1.1) (size 1.7 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 02582e87-7f36-451a-8fdc-5e003e7b03c7))
  (pad "2" smd roundrect (at -1.5 1.1) (size 1.7 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 9fb17bd7-6f17-4efb-a2e5-2c1c01abe4f2))
  (pad "3" smd roundrect (at 1.5 1.1) (size 1.7 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp f7ca433b-e2fe-4728-8c74-c4df259907b7))
  (pad "4" smd roundrect (at 1.5 -1.1) (size 1.7 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp c2203508-36eb-479c-b89c-28088d985aba))
  (model "${KIPRJMOD}/Yellow.3dshapes/L_CommonModeChoke_Murata_DLW5B.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
