(footprint "L_Bourns-SDR1006" (version 20210108) (generator pcbnew) (layer "F.Cu")
  (tedit 601047B2)
  (descr "Bourns SDR1006 series SMD inductor https://www.bourns.com/docs/Product-Datasheets/SDR1006.pdf")
  (tags "Bourns SDR1006 SMD inductor")
  (attr smd)
  (fp_text reference "REF**" (at 0 -6.2) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 81a5d54d-0a13-4dc5-90a5-d1c09e6a0123)
  )
  (fp_text value "L_Bourns-SDR1006" (at 0 6.2) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp fd8f2b3e-3b1f-4764-9b3b-b2c96679d250)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 4dfee27a-8683-449c-83a8-5bfc3ad172f7)
  )
  (fp_line (start 5.31 5.36) (end 3.81 5.36) (layer "F.SilkS") (width 0.12) (tstamp 1dcb87ee-29e3-4f64-90f7-272f32f49d22))
  (fp_line (start -5.31 5.36) (end -3.81 5.36) (layer "F.SilkS") (width 0.12) (tstamp 2357e092-0641-4d86-8480-8d0eac587477))
  (fp_line (start 5.31 5.36) (end 5.31 3.86) (layer "F.SilkS") (width 0.12) (tstamp 43837fc2-3b10-4603-93e5-9e8f3494cb59))
  (fp_line (start 5.31 -5.36) (end 3.81 -5.36) (layer "F.SilkS") (width 0.12) (tstamp 70fe6a95-d276-43cc-ac20-047afada68d3))
  (fp_line (start -5.31 5.36) (end -5.31 3.86) (layer "F.SilkS") (width 0.12) (tstamp 7e1183ad-4b7a-4b88-b3c9-b1cde320f2b5))
  (fp_line (start -5.31 -5.36) (end -3.81 -5.36) (layer "F.SilkS") (width 0.12) (tstamp d17b0a70-b91f-44ee-a507-db2469b8234a))
  (fp_line (start -5.31 -5.36) (end -5.31 -3.86) (layer "F.SilkS") (width 0.12) (tstamp d3ffa8f9-e39b-4efd-b801-9af3f5d6de86))
  (fp_line (start 5.31 -5.36) (end 5.31 -3.86) (layer "F.SilkS") (width 0.12) (tstamp f374a435-76a9-4234-a4a4-800f993c262b))
  (fp_line (start 5.3 -5.35) (end 5.3 5.35) (layer "F.CrtYd") (width 0.05) (tstamp 383ae993-d31a-40c9-9195-f3ece28a0ac2))
  (fp_line (start -5.3 5.35) (end 5.3 5.35) (layer "F.CrtYd") (width 0.05) (tstamp 5e274b9e-57cf-45b1-9276-aef56b09d937))
  (fp_line (start -5.3 -5.35) (end -5.3 5.35) (layer "F.CrtYd") (width 0.05) (tstamp 887377d1-19c6-4513-bd16-8968755a4b82))
  (fp_line (start -5.3 -5.35) (end 5.3 -5.35) (layer "F.CrtYd") (width 0.05) (tstamp a5c73267-aa4e-4831-b2e7-26fb25bd793a))
  (fp_circle (center 0 0) (end 4.9 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp dba8fc0d-dacf-4cf1-b24c-166ea9de9e07))
  (pad "1" smd roundrect (at -3.2 0) (locked) (size 3.6 10) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0) (chamfer top_right bottom_right) (tstamp a3a3c313-b7b6-4033-b4e6-382dc449099f))
  (pad "2" smd roundrect (at 3.2 0) (locked) (size 3.6 10) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0) (chamfer top_left bottom_left) (tstamp 6c66381e-ef84-4e9a-b1d6-81c359f0ff75))
  (model "${KISYS3DMOD}/Inductor_SMD.3dshapes/L_Bourns-SRN1060.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
