<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.1">
<drawing>
<library>
<packages>
<package name="RPI3">
<description>Package for the Raspberry Pi 3 board created by Dave Young for www.elemenet14.com based on documented dimensions and board measurements.
For more documentation, please visit http://www.raspberrypi.org/documentation/hardware/raspberrypi/</description>
</package>
<package name="RPI3-NO-CONNECTORS">
</package>
</packages>
<symbols>
<symbol name="RPI3">
<description>Symbol for the Raspberry Pi 3 Single Board Computer created by Dave Young for www.element14.com
For more documentation, visit http://www.raspberrypi.org/documentation/hardware/raspberrypi/</description>
<pin name="3V3@1"/>
<pin name="5V@2"/>
<pin name="GPIO2"/>
<pin name="5V@4"/>
<pin name="GPIO3"/>
<pin name="GND@6"/>
<pin name="GPIO4"/>
<pin name="GPIO14"/>
<pin name="GND@9"/>
<pin name="GPIO15"/>
<pin name="GPIO17"/>
<pin name="GPIO18"/>
<pin name="GPIO27"/>
<pin name="GND@14"/>
<pin name="GPIO22"/>
<pin name="GPIO23"/>
<pin name="3V3@17"/>
<pin name="GPIO24"/>
<pin name="GPIO10"/>
<pin name="GND@20"/>
<pin name="GPIO9"/>
<pin name="GPIO25"/>
<pin name="GPIO11"/>
<pin name="GPIO8"/>
<pin name="GND@25"/>
<pin name="GPIO7"/>
<pin name="ID_SD*"/>
<pin name="ID_SC*"/>
<pin name="GPIO5"/>
<pin name="GND@30"/>
<pin name="GPIO6"/>
<pin name="GPIO12"/>
<pin name="GPIO13"/>
<pin name="GND@34"/>
<pin name="GPIO19"/>
<pin name="GPIO16"/>
<pin name="GPIO26"/>
<pin name="GPIO20"/>
<pin name="GND@39"/>
<pin name="GPIO21"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="RPI3" prefix="PCB">
<description>Device for Raspberry Pi 3 board created by Dave Young for www.element14.com
More information and support community is available at https://www.element14.com/community/community/raspberry-pi</description>
<gates>
<gate name="G$1" symbol="RPI3"/>
</gates>
<devices>
<device name="" package="RPI3">
<connects>
<connect gate="G$1" pin="3V3@1" pad="P$1"/>
<connect gate="G$1" pin="3V3@17" pad="P$17"/>
<connect gate="G$1" pin="5V@2" pad="P$2"/>
<connect gate="G$1" pin="5V@4" pad="P$4"/>
<connect gate="G$1" pin="GND@14" pad="P$14"/>
<connect gate="G$1" pin="GND@20" pad="P$20"/>
<connect gate="G$1" pin="GND@25" pad="P$25"/>
<connect gate="G$1" pin="GND@30" pad="P$30"/>
<connect gate="G$1" pin="GND@34" pad="P$34"/>
<connect gate="G$1" pin="GND@39" pad="P$39"/>
<connect gate="G$1" pin="GND@6" pad="P$6"/>
<connect gate="G$1" pin="GND@9" pad="P$9"/>
<connect gate="G$1" pin="GPIO10" pad="P$19"/>
<connect gate="G$1" pin="GPIO11" pad="P$23"/>
<connect gate="G$1" pin="GPIO12" pad="P$32"/>
<connect gate="G$1" pin="GPIO13" pad="P$33"/>
<connect gate="G$1" pin="GPIO14" pad="P$8"/>
<connect gate="G$1" pin="GPIO15" pad="P$10"/>
<connect gate="G$1" pin="GPIO16" pad="P$36"/>
<connect gate="G$1" pin="GPIO17" pad="P$11"/>
<connect gate="G$1" pin="GPIO18" pad="P$12"/>
<connect gate="G$1" pin="GPIO19" pad="P$35"/>
<connect gate="G$1" pin="GPIO2" pad="P$3"/>
<connect gate="G$1" pin="GPIO20" pad="P$38"/>
<connect gate="G$1" pin="GPIO21" pad="P$40"/>
<connect gate="G$1" pin="GPIO22" pad="P$15"/>
<connect gate="G$1" pin="GPIO23" pad="P$16"/>
<connect gate="G$1" pin="GPIO24" pad="P$18"/>
<connect gate="G$1" pin="GPIO25" pad="P$22"/>
<connect gate="G$1" pin="GPIO26" pad="P$37"/>
<connect gate="G$1" pin="GPIO27" pad="P$13"/>
<connect gate="G$1" pin="GPIO3" pad="P$5"/>
<connect gate="G$1" pin="GPIO4" pad="P$7"/>
<connect gate="G$1" pin="GPIO5" pad="P$29"/>
<connect gate="G$1" pin="GPIO6" pad="P$31"/>
<connect gate="G$1" pin="GPIO7" pad="P$26"/>
<connect gate="G$1" pin="GPIO8" pad="P$24"/>
<connect gate="G$1" pin="GPIO9" pad="P$21"/>
<connect gate="G$1" pin="ID_SC*" pad="P$28"/>
<connect gate="G$1" pin="ID_SD*" pad="P$27"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NO-CONNECTORS" package="RPI3-NO-CONNECTORS">
<connects>
<connect gate="G$1" pin="3V3@1" pad="P$1"/>
<connect gate="G$1" pin="3V3@17" pad="P$17"/>
<connect gate="G$1" pin="5V@2" pad="P$2"/>
<connect gate="G$1" pin="5V@4" pad="P$4"/>
<connect gate="G$1" pin="GND@14" pad="P$14"/>
<connect gate="G$1" pin="GND@20" pad="P$20"/>
<connect gate="G$1" pin="GND@25" pad="P$25"/>
<connect gate="G$1" pin="GND@30" pad="P$30"/>
<connect gate="G$1" pin="GND@34" pad="P$34"/>
<connect gate="G$1" pin="GND@39" pad="P$39"/>
<connect gate="G$1" pin="GND@6" pad="P$6"/>
<connect gate="G$1" pin="GND@9" pad="P$9"/>
<connect gate="G$1" pin="GPIO10" pad="P$19"/>
<connect gate="G$1" pin="GPIO11" pad="P$23"/>
<connect gate="G$1" pin="GPIO12" pad="P$32"/>
<connect gate="G$1" pin="GPIO13" pad="P$33"/>
<connect gate="G$1" pin="GPIO14" pad="P$8"/>
<connect gate="G$1" pin="GPIO15" pad="P$10"/>
<connect gate="G$1" pin="GPIO16" pad="P$36"/>
<connect gate="G$1" pin="GPIO17" pad="P$11"/>
<connect gate="G$1" pin="GPIO18" pad="P$12"/>
<connect gate="G$1" pin="GPIO19" pad="P$35"/>
<connect gate="G$1" pin="GPIO2" pad="P$3"/>
<connect gate="G$1" pin="GPIO20" pad="P$38"/>
<connect gate="G$1" pin="GPIO21" pad="P$40"/>
<connect gate="G$1" pin="GPIO22" pad="P$15"/>
<connect gate="G$1" pin="GPIO23" pad="P$16"/>
<connect gate="G$1" pin="GPIO24" pad="P$18"/>
<connect gate="G$1" pin="GPIO25" pad="P$22"/>
<connect gate="G$1" pin="GPIO26" pad="P$37"/>
<connect gate="G$1" pin="GPIO27" pad="P$13"/>
<connect gate="G$1" pin="GPIO3" pad="P$5"/>
<connect gate="G$1" pin="GPIO4" pad="P$7"/>
<connect gate="G$1" pin="GPIO5" pad="P$29"/>
<connect gate="G$1" pin="GPIO6" pad="P$31"/>
<connect gate="G$1" pin="GPIO7" pad="P$26"/>
<connect gate="G$1" pin="GPIO8" pad="P$24"/>
<connect gate="G$1" pin="GPIO9" pad="P$21"/>
<connect gate="G$1" pin="ID_SC*" pad="P$28"/>
<connect gate="G$1" pin="ID_SD*" pad="P$27"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
