(export (version D)
  (design
    (source /root/rgb2svid/rgb2svid.sch)
    (date "Tue Aug 28 02:29:10 2018")
    (tool "Eeschema (5.0.0)")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title "RGB to Component/S-Video/Composite Converter")
        (company "Scott Alfter")
        (rev 0.1)
        (date 2018-02-22)
        (source rgb2svid.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 2) (name /rgb2component/) (tstamps /5A8FE7B6/)
      (title_block
        (title "RGB to Component/S-Video/Composite Converter")
        (company "Scott Alfter")
        (rev 0.1)
        (date 2018-02-22)
        (source rgb2component.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 3) (name /oscillator/) (tstamps /5A932E50/)
      (title_block
        (title "RGB to Component/S-Video/Composite Converter")
        (company "Scott Alfter")
        (rev 0.1)
        (date 2018-02-25)
        (source osc.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref J1)
      (value IIGS_RGB)
      (footprint Connector_Dsub:DSUB-15_Male_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm)
      (libsource (lib apple2) (part IIGS_RGB) (description "Apple IIGS RGB output"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A8F9E87))
    (comp (ref C2)
      (value 0.1u)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet http://www.samsungsem.com/kr/support/product-search/mlcc/CL21F104ZBCNNNC.jsp)
      (fields
        (field (name Description) "CAP CER 0.1UF 50V Y5V 0805")
        (field (name "JEDEC Pkg") 0805)
        (field (name Manufacturer) "Samsung Electro-Mechanics")
        (field (name "Mfr PN") CL21F104ZBCNNNC)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") 1276-1007-1-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=1276-1007-1-ND))
      (libsource (lib proper-passives) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A8F9FD5))
    (comp (ref C4)
      (value 0.1u)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet http://www.samsungsem.com/kr/support/product-search/mlcc/CL21F104ZBCNNNC.jsp)
      (fields
        (field (name Description) "CAP CER 0.1UF 50V Y5V 0805")
        (field (name "JEDEC Pkg") 0805)
        (field (name Manufacturer) "Samsung Electro-Mechanics")
        (field (name "Mfr PN") CL21F104ZBCNNNC)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") 1276-1007-1-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=1276-1007-1-ND))
      (libsource (lib proper-passives) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A8FA149))
    (comp (ref C5)
      (value 0.1u)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet http://www.samsungsem.com/kr/support/product-search/mlcc/CL21F104ZBCNNNC.jsp)
      (fields
        (field (name Description) "CAP CER 0.1UF 50V Y5V 0805")
        (field (name "JEDEC Pkg") 0805)
        (field (name Manufacturer) "Samsung Electro-Mechanics")
        (field (name "Mfr PN") CL21F104ZBCNNNC)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") 1276-1007-1-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=1276-1007-1-ND))
      (libsource (lib proper-passives) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A8FA239))
    (comp (ref U1)
      (value L7805)
      (footprint Package_TO_SOT_SMD:TO-252-2)
      (datasheet http://www.st.com/content/ccc/resource/technical/document/datasheet/41/4f/b3/b0/12/d4/47/88/CD00000444.pdf/files/CD00000444.pdf/jcr:content/translations/en.CD00000444.pdf)
      (fields
        (field (name Description) "IC REG LINEAR 5V 1.5A DPAK")
        (field (name "JEDEC Pkg") TO-252-2)
        (field (name Manufacturer) ST)
        (field (name "Mfr PN") L7805CDT-TR)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") 497-7255-1-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=497-7255-1-ND))
      (libsource (lib rgb2svid-rescue) (part L7805) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A8FA5BA))
    (comp (ref C1)
      (value 0.1u)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet http://www.samsungsem.com/kr/support/product-search/mlcc/CL21F104ZBCNNNC.jsp)
      (fields
        (field (name Description) "CAP CER 0.1UF 50V Y5V 0805")
        (field (name "JEDEC Pkg") 0805)
        (field (name Manufacturer) "Samsung Electro-Mechanics")
        (field (name "Mfr PN") CL21F104ZBCNNNC)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") 1276-1007-1-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=1276-1007-1-ND))
      (libsource (lib proper-passives) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A8FA68B))
    (comp (ref C3)
      (value 1u)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet http://www.samsungsem.com/kr/support/product-search/mlcc/CL21F105ZOCNNNC.jsp)
      (fields
        (field (name Description) "CAP CER 1UF 16V Y5V 0805")
        (field (name "JEDEC Pkg") 0805)
        (field (name Manufacturer) "Samsung Electro-Mechanics")
        (field (name "Mfr PN") CL21F105ZOCNNNC)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") 1276-1246-1-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=1276-1246-1-ND))
      (libsource (lib proper-passives) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A8FA724))
    (comp (ref R1)
      (value 3.32k)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet https://www.seielect.com/Catalog/SEI-RMCF_RMCP.pdf)
      (fields
        (field (name Description) "RES 3.32K OHM 1% 1/8W 0805")
        (field (name "JEDEC Pkg") 0805)
        (field (name Manufacturer) "Stackpole Electronics Inc.")
        (field (name "Mfr PN") RMCF0805FT3K32)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") RMCF0805FT3K32CT-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=RMCF0805FT3K32CT-ND))
      (libsource (lib proper-passives) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A8FBED7))
    (comp (ref R3)
      (value 75)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet https://www.seielect.com/Catalog/SEI-RMCF_RMCP.pdf)
      (fields
        (field (name Description) "RES 75 OHM 1% 1/8W 0805")
        (field (name "JEDEC Pkg") 0805)
        (field (name Manufacturer) "Stackpole Electronics Inc.")
        (field (name "Mfr PN") RMCF0805FT75R0)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") RMCF0805FT75R0CT-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=RMCF0805FT75R0CT-ND))
      (libsource (lib proper-passives) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A8FC60C))
    (comp (ref R4)
      (value 75)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet https://www.seielect.com/Catalog/SEI-RMCF_RMCP.pdf)
      (fields
        (field (name Description) "RES 75 OHM 1% 1/8W 0805")
        (field (name "JEDEC Pkg") 0805)
        (field (name Manufacturer) "Stackpole Electronics Inc.")
        (field (name "Mfr PN") RMCF0805FT75R0)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") RMCF0805FT75R0CT-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=RMCF0805FT75R0CT-ND))
      (libsource (lib proper-passives) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A8FC706))
    (comp (ref C11)
      (value 220u)
      (footprint Capacitor_Tantalum_SMD:CP_EIA-3528-12_Kemet-T)
      (datasheet http://datasheets.avx.com/F93.pdf)
      (fields
        (field (name Description) "CAP TANT 220UF 6.3V 10% 1411")
        (field (name "JEDEC Pkg") 1411)
        (field (name Manufacturer) "AVX Corporation")
        (field (name "Mfr PN") F930J227KBA)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") 478-8166-1-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=478-8166-1-ND))
      (libsource (lib proper-passives) (part CP) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A8FC7C9))
    (comp (ref C12)
      (value 220u)
      (footprint Capacitor_Tantalum_SMD:CP_EIA-3528-12_Kemet-T)
      (datasheet http://datasheets.avx.com/F93.pdf)
      (fields
        (field (name Description) "CAP TANT 220UF 6.3V 10% 1411")
        (field (name "JEDEC Pkg") 1411)
        (field (name Manufacturer) "AVX Corporation")
        (field (name "Mfr PN") F930J227KBA)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") 478-8166-1-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=478-8166-1-ND))
      (libsource (lib proper-passives) (part CP) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A8FC8F8))
    (comp (ref C7)
      (value 0.01u)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet http://www.samsungsem.com/kr/support/product-search/mlcc/CL21F103ZBANNNC.jsp)
      (fields
        (field (name Description) "CAP CER 10000PF 50V Y5V 0805")
        (field (name "JEDEC Pkg") 0805)
        (field (name Manufacturer) "Samsung Electro-Mechanics")
        (field (name "Mfr PN") CL21F103ZBANNNC)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") 1276-2705-1-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=1276-2705-1-ND))
      (libsource (lib proper-passives) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A8FCD09))
    (comp (ref C6)
      (value 470u)
      (footprint Capacitor_Tantalum_SMD:CP_EIA-7343-20_Kemet-V)
      (datasheet http://www.vishay.com/docs/40002/293d.pdf)
      (fields
        (field (name Description) "CAP TANT 470UF 6.3V 10% 2917")
        (field (name "JEDEC Pkg") 2917)
        (field (name Manufacturer) "Vishay Sprague")
        (field (name "Mfr PN") 293D477X96R3D2TE3)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") 718-1749-1-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=718-1749-1-ND))
      (libsource (lib proper-passives) (part CP) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A8FCE52))
    (comp (ref C8)
      (value 0.01u)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet http://www.samsungsem.com/kr/support/product-search/mlcc/CL21F103ZBANNNC.jsp)
      (fields
        (field (name Description) "CAP CER 10000PF 50V Y5V 0805")
        (field (name "JEDEC Pkg") 0805)
        (field (name Manufacturer) "Samsung Electro-Mechanics")
        (field (name "Mfr PN") CL21F103ZBANNNC)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") 1276-2705-1-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=1276-2705-1-ND))
      (libsource (lib proper-passives) (part C) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A8FD0F2))
    (comp (ref C9)
      (value 470u)
      (footprint Capacitor_Tantalum_SMD:CP_EIA-7343-20_Kemet-V)
      (datasheet http://www.vishay.com/docs/40002/293d.pdf)
      (fields
        (field (name Description) "CAP TANT 470UF 6.3V 10% 2917")
        (field (name "JEDEC Pkg") 2917)
        (field (name Manufacturer) "Vishay Sprague")
        (field (name "Mfr PN") 293D477X96R3D2TE3)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") 718-1749-1-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=718-1749-1-ND))
      (libsource (lib proper-passives) (part CP) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A8FD13D))
    (comp (ref U2)
      (value CXA2075)
      (footprint sop:SOP-24_15.0x5.3mm_P1.27mm)
      (datasheet http://pdf1.alldatasheet.com/datasheet-pdf/view/146350/SONY/CXA2075M/+0_5473VPMMZb.a.NBEDU+/datasheet.pdf)
      (fields
        (field (name Description) "RGB Encoder")
        (field (name Manufacturer) Sony)
        (field (name "Mfr PN") CXA2075M)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") n))
      (libsource (lib cxa1645) (part CXA2075) (description "RGB to NTSC/PAL encoder"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A8FDC56))
    (comp (ref J3)
      (value S-Video)
      (footprint conns:mini-din-4)
      (datasheet https://www.cui.com/product/resource/md-s.pdf)
      (fields
        (field (name Description) https://www.digikey.com/products/en?keywords=CP-2440-ND)
        (field (name Manufacturer) "CUI Inc.")
        (field (name "Mfr PN") MD-40S)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") CP-2440-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=CP-2440-ND))
      (libsource (lib rgb2svid-rescue) (part Mini-DIN-4) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A8FDFCE))
    (comp (ref R2)
      (value 75)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet https://www.seielect.com/Catalog/SEI-RMCF_RMCP.pdf)
      (fields
        (field (name Description) "RES 75 OHM 1% 1/8W 0805")
        (field (name "JEDEC Pkg") 0805)
        (field (name Manufacturer) "Stackpole Electronics Inc.")
        (field (name "Mfr PN") RMCF0805FT75R0)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") RMCF0805FT75R0CT-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=RMCF0805FT75R0CT-ND))
      (libsource (lib proper-passives) (part R) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A8FE2F9))
    (comp (ref C10)
      (value 220u)
      (footprint Capacitor_Tantalum_SMD:CP_EIA-3528-12_Kemet-T)
      (datasheet http://datasheets.avx.com/F93.pdf)
      (fields
        (field (name Description) "CAP TANT 220UF 6.3V 10% 1411")
        (field (name "JEDEC Pkg") 1411)
        (field (name Manufacturer) "AVX Corporation")
        (field (name "Mfr PN") F930J227KBA)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") 478-8166-1-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=478-8166-1-ND))
      (libsource (lib proper-passives) (part CP) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A8FE349))
    (comp (ref J2)
      (value Composite)
      (footprint conns:rca-right-angle)
      (datasheet http://www.switchcraft.com/Drawings/pjran1x1u__x_series_cd.pdf)
      (fields
        (field (name Description) "CONN RCA JACK MONO 3.2MM R/A")
        (field (name Manufacturer) "Switchcraft Inc.")
        (field (name "Mfr PN") PJRAN1X1U04X)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") PJRAN1X1U04X-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=PJRAN1X1U04X-ND))
      (libsource (lib rgb2svid-rescue) (part Conn_Coaxial) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A8FE45C))
    (comp (ref U4)
      (value via)
      (footprint thermal-vias:via-25mil)
      (libsource (lib via) (part via) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A934273))
    (comp (ref U5)
      (value via)
      (footprint thermal-vias:via-25mil)
      (libsource (lib via) (part via) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A934476))
    (comp (ref U6)
      (value via)
      (footprint thermal-vias:via-25mil)
      (libsource (lib via) (part via) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A93450B))
    (comp (ref U7)
      (value via)
      (footprint thermal-vias:via-25mil)
      (libsource (lib via) (part via) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A934518))
    (comp (ref U8)
      (value via)
      (footprint thermal-vias:via-25mil)
      (libsource (lib via) (part via) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A93504D))
    (comp (ref U9)
      (value via)
      (footprint thermal-vias:via-25mil)
      (libsource (lib via) (part via) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A93505A))
    (comp (ref U10)
      (value via)
      (footprint thermal-vias:via-25mil)
      (libsource (lib via) (part via) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A935067))
    (comp (ref U11)
      (value via)
      (footprint thermal-vias:via-25mil)
      (libsource (lib via) (part via) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A935074))
    (comp (ref U12)
      (value via)
      (footprint thermal-vias:via-25mil)
      (libsource (lib via) (part via) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A935109))
    (comp (ref JP1)
      (value Jumper_NC_Small)
      (footprint jumpers:jumper_nc)
      (libsource (lib Device) (part Jumper_NC_Small) (description "Jumper, normally closed"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A9363C5))
    (comp (ref JP2)
      (value Jumper_NO_Small)
      (footprint jumpers:jumper_no)
      (libsource (lib Device) (part Jumper_NO_Small) (description "Jumper, normally open"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A9366D3))
    (comp (ref U14)
      (value via)
      (footprint untented-vias:via-untented-15-25)
      (libsource (lib via) (part via) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A9380C6))
    (comp (ref U15)
      (value via)
      (footprint untented-vias:via-untented-15-25)
      (libsource (lib via) (part via) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A9384DB))
    (comp (ref U16)
      (value via)
      (footprint untented-vias:via-untented-15-25)
      (libsource (lib via) (part via) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A938549))
    (comp (ref U17)
      (value via)
      (footprint untented-vias:via-untented-15-25)
      (libsource (lib via) (part via) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A9385B7))
    (comp (ref U18)
      (value via)
      (footprint untented-vias:via-untented-15-25)
      (libsource (lib via) (part via) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A938625))
    (comp (ref U19)
      (value via)
      (footprint untented-vias:via-untented-15-25)
      (libsource (lib via) (part via) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A938693))
    (comp (ref C13)
      (value 100u)
      (footprint Capacitor_Tantalum_SMD:CP_EIA-3528-12_Kemet-T)
      (datasheet http://datasheets.avx.com/F93.pdf)
      (fields
        (field (name Description) "CAP TANT 100UF 6.3V 20% 1411")
        (field (name "JEDEC Pkg") 1411)
        (field (name Manufacturer) "AVX Corporation")
        (field (name "Mfr PN") F930J107MBA)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") 478-8156-1-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=478-8156-1-ND))
      (libsource (lib proper-passives) (part CP) (description ""))
      (sheetpath (names /rgb2component/) (tstamps /5A8FE7B6/))
      (tstamp 5A90032F))
    (comp (ref R5)
      (value 680)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet https://www.seielect.com/Catalog/SEI-RMCF_RMCP.pdf)
      (fields
        (field (name Description) "RES 680 OHM 1% 1/8W 0805")
        (field (name "JEDEC Pkg") 0805)
        (field (name Manufacturer) "Stackpole Electronics Inc.")
        (field (name "Mfr PN") RMCF0805FT680R)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") RMCF0805FT680RCT-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=RMCF0805FT680RCT-ND))
      (libsource (lib proper-passives) (part R) (description ""))
      (sheetpath (names /rgb2component/) (tstamps /5A8FE7B6/))
      (tstamp 5A9003AE))
    (comp (ref R7)
      (value 82)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet https://www.seielect.com/Catalog/SEI-RMCF_RMCP.pdf)
      (fields
        (field (name Description) "RES 82 OHM 1% 1/8W 0805")
        (field (name "JEDEC Pkg") 0805)
        (field (name Manufacturer) "Stackpole Electronics Inc.")
        (field (name "Mfr PN") RMCF0805FT82R0)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") RMCF0805FT82R0CT-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=RMCF0805FT82R0CT-ND))
      (libsource (lib proper-passives) (part R) (description ""))
      (sheetpath (names /rgb2component/) (tstamps /5A8FE7B6/))
      (tstamp 5A9003EF))
    (comp (ref R8)
      (value 91)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet https://www.seielect.com/Catalog/SEI-RMCF_RMCP.pdf)
      (fields
        (field (name Description) "RES 91 OHM 1% 1/8W 0805")
        (field (name "JEDEC Pkg") 0805)
        (field (name Manufacturer) "Stackpole Electronics Inc.")
        (field (name "Mfr PN") RMCF0805FT91R0)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") RMCF0805FT91R0CT-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=RMCF0805FT91R0CT-ND))
      (libsource (lib proper-passives) (part R) (description ""))
      (sheetpath (names /rgb2component/) (tstamps /5A8FE7B6/))
      (tstamp 5A9004B4))
    (comp (ref R6)
      (value 91)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet https://www.seielect.com/Catalog/SEI-RMCF_RMCP.pdf)
      (fields
        (field (name Description) "RES 91 OHM 1% 1/8W 0805")
        (field (name "JEDEC Pkg") 0805)
        (field (name Manufacturer) "Stackpole Electronics Inc.")
        (field (name "Mfr PN") RMCF0805FT91R0)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") RMCF0805FT91R0CT-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=RMCF0805FT91R0CT-ND))
      (libsource (lib proper-passives) (part R) (description ""))
      (sheetpath (names /rgb2component/) (tstamps /5A8FE7B6/))
      (tstamp 5A90058B))
    (comp (ref R9)
      (value 866)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet https://www.seielect.com/Catalog/SEI-RMCF_RMCP.pdf)
      (fields
        (field (name Description) "RES 866 OHM 1% 1/8W 0805")
        (field (name "JEDEC Pkg") 0805)
        (field (name Manufacturer) "Stackpole Electronics Inc.")
        (field (name "Mfr PN") RMCF0805FT866R)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") RMCF0805FT866RCT-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=RMCF0805FT866RCT-ND))
      (libsource (lib proper-passives) (part R) (description ""))
      (sheetpath (names /rgb2component/) (tstamps /5A8FE7B6/))
      (tstamp 5A900666))
    (comp (ref R10)
      (value 1.69k)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet https://www.seielect.com/Catalog/SEI-RMCF_RMCP.pdf)
      (fields
        (field (name Description) "RES 1.69K OHM 1% 1/8W 0805")
        (field (name "JEDEC Pkg") 0805)
        (field (name Manufacturer) "Stackpole Electronics Inc.")
        (field (name "Mfr PN") RMCF0805FT1K69)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") RMCF0805FT1K69CT-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=RMCF0805FT1K69CT-ND))
      (libsource (lib proper-passives) (part R) (description ""))
      (sheetpath (names /rgb2component/) (tstamps /5A8FE7B6/))
      (tstamp 5A900756))
    (comp (ref R11)
      (value 4.64k)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet https://www.seielect.com/Catalog/SEI-RMCF_RMCP.pdf)
      (fields
        (field (name Description) "RES 4.64K OHM 1% 1/8W 0805")
        (field (name "JEDEC Pkg") 0805)
        (field (name Manufacturer) "Stackpole Electronics Inc.")
        (field (name "Mfr PN") RMCF0805FT4K64)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") RMCF0805FT4K64CT-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=RMCF0805FT4K64CT-ND))
      (libsource (lib proper-passives) (part R) (description ""))
      (sheetpath (names /rgb2component/) (tstamps /5A8FE7B6/))
      (tstamp 5A9007CE))
    (comp (ref U3)
      (value MAX4383)
      (footprint Package_SO:SOIC-14_3.9x8.7mm_P1.27mm)
      (datasheet https://datasheets.maximintegrated.com/en/ds/MAX4380-MAX4384.pdf)
      (fields
        (field (name Description) "IC OPAMP VFB 210MHZ RRO 14SOIC")
        (field (name "JEDEC Pkg") SOIC-14)
        (field (name Manufacturer) "Maxim Integrated")
        (field (name "Mfr PN") MAX4383ESD+)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") n)
        (field (name "Vendor 1 PN") MAX4383ESD+-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=MAX4383ESD+-ND))
      (libsource (lib rgb2svid-rescue) (part MC33079) (description ""))
      (sheetpath (names /rgb2component/) (tstamps /5A8FE7B6/))
      (tstamp 5A90087A))
    (comp (ref R14)
      (value 510)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet https://www.seielect.com/Catalog/SEI-RMCF_RMCP.pdf)
      (fields
        (field (name Description) "RES 510 OHM 1% 1/8W 0805")
        (field (name "JEDEC Pkg") 0805)
        (field (name Manufacturer) "Stackpole Electronics Inc.")
        (field (name "Mfr PN") RMCF0805FT510R)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") RMCF0805FT510RCT-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=RMCF0805FT510RCT-ND))
      (libsource (lib proper-passives) (part R) (description ""))
      (sheetpath (names /rgb2component/) (tstamps /5A8FE7B6/))
      (tstamp 5A900C6B))
    (comp (ref C14)
      (value 0.1u)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet http://www.samsungsem.com/kr/support/product-search/mlcc/CL21F104ZBCNNNC.jsp)
      (fields
        (field (name Description) "CAP CER 0.1UF 50V Y5V 0805")
        (field (name "JEDEC Pkg") 0805)
        (field (name Manufacturer) "Samsung Electro-Mechanics")
        (field (name "Mfr PN") CL21F104ZBCNNNC)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") 1276-1007-1-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=1276-1007-1-ND))
      (libsource (lib proper-passives) (part C) (description ""))
      (sheetpath (names /rgb2component/) (tstamps /5A8FE7B6/))
      (tstamp 5A900E2E))
    (comp (ref R13)
      (value 510)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet https://www.seielect.com/Catalog/SEI-RMCF_RMCP.pdf)
      (fields
        (field (name Description) "RES 510 OHM 1% 1/8W 0805")
        (field (name "JEDEC Pkg") 0805)
        (field (name Manufacturer) "Stackpole Electronics Inc.")
        (field (name "Mfr PN") RMCF0805FT510R)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") RMCF0805FT510RCT-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=RMCF0805FT510RCT-ND))
      (libsource (lib proper-passives) (part R) (description ""))
      (sheetpath (names /rgb2component/) (tstamps /5A8FE7B6/))
      (tstamp 5A900F8D))
    (comp (ref R12)
      (value 510)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet https://www.seielect.com/Catalog/SEI-RMCF_RMCP.pdf)
      (fields
        (field (name Description) "RES 510 OHM 1% 1/8W 0805")
        (field (name "JEDEC Pkg") 0805)
        (field (name Manufacturer) "Stackpole Electronics Inc.")
        (field (name "Mfr PN") RMCF0805FT510R)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") RMCF0805FT510RCT-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=RMCF0805FT510RCT-ND))
      (libsource (lib proper-passives) (part R) (description ""))
      (sheetpath (names /rgb2component/) (tstamps /5A8FE7B6/))
      (tstamp 5A901016))
    (comp (ref R15)
      (value 510)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet https://www.seielect.com/Catalog/SEI-RMCF_RMCP.pdf)
      (fields
        (field (name Description) "RES 510 OHM 1% 1/8W 0805")
        (field (name "JEDEC Pkg") 0805)
        (field (name Manufacturer) "Stackpole Electronics Inc.")
        (field (name "Mfr PN") RMCF0805FT510R)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") RMCF0805FT510RCT-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=RMCF0805FT510RCT-ND))
      (libsource (lib proper-passives) (part R) (description ""))
      (sheetpath (names /rgb2component/) (tstamps /5A8FE7B6/))
      (tstamp 5A901112))
    (comp (ref R16)
      (value 510)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet https://www.seielect.com/Catalog/SEI-RMCF_RMCP.pdf)
      (fields
        (field (name Description) "RES 510 OHM 1% 1/8W 0805")
        (field (name "JEDEC Pkg") 0805)
        (field (name Manufacturer) "Stackpole Electronics Inc.")
        (field (name "Mfr PN") RMCF0805FT510R)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") RMCF0805FT510RCT-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=RMCF0805FT510RCT-ND))
      (libsource (lib proper-passives) (part R) (description ""))
      (sheetpath (names /rgb2component/) (tstamps /5A8FE7B6/))
      (tstamp 5A90116F))
    (comp (ref R17)
      (value 510)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet https://www.seielect.com/Catalog/SEI-RMCF_RMCP.pdf)
      (fields
        (field (name Description) "RES 510 OHM 1% 1/8W 0805")
        (field (name "JEDEC Pkg") 0805)
        (field (name Manufacturer) "Stackpole Electronics Inc.")
        (field (name "Mfr PN") RMCF0805FT510R)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") RMCF0805FT510RCT-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=RMCF0805FT510RCT-ND))
      (libsource (lib proper-passives) (part R) (description ""))
      (sheetpath (names /rgb2component/) (tstamps /5A8FE7B6/))
      (tstamp 5A9012C5))
    (comp (ref R18)
      (value 510)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet https://www.seielect.com/Catalog/SEI-RMCF_RMCP.pdf)
      (fields
        (field (name Description) "RES 510 OHM 1% 1/8W 0805")
        (field (name "JEDEC Pkg") 0805)
        (field (name Manufacturer) "Stackpole Electronics Inc.")
        (field (name "Mfr PN") RMCF0805FT510R)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") RMCF0805FT510RCT-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=RMCF0805FT510RCT-ND))
      (libsource (lib proper-passives) (part R) (description ""))
      (sheetpath (names /rgb2component/) (tstamps /5A8FE7B6/))
      (tstamp 5A9019DC))
    (comp (ref R21)
      (value 510)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet https://www.seielect.com/Catalog/SEI-RMCF_RMCP.pdf)
      (fields
        (field (name Description) "RES 510 OHM 1% 1/8W 0805")
        (field (name "JEDEC Pkg") 0805)
        (field (name Manufacturer) "Stackpole Electronics Inc.")
        (field (name "Mfr PN") RMCF0805FT510R)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") RMCF0805FT510RCT-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=RMCF0805FT510RCT-ND))
      (libsource (lib proper-passives) (part R) (description ""))
      (sheetpath (names /rgb2component/) (tstamps /5A8FE7B6/))
      (tstamp 5A903A6B))
    (comp (ref R22)
      (value 510)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet https://www.seielect.com/Catalog/SEI-RMCF_RMCP.pdf)
      (fields
        (field (name Description) "RES 510 OHM 1% 1/8W 0805")
        (field (name "JEDEC Pkg") 0805)
        (field (name Manufacturer) "Stackpole Electronics Inc.")
        (field (name "Mfr PN") RMCF0805FT510R)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") RMCF0805FT510RCT-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=RMCF0805FT510RCT-ND))
      (libsource (lib proper-passives) (part R) (description ""))
      (sheetpath (names /rgb2component/) (tstamps /5A8FE7B6/))
      (tstamp 5A903B22))
    (comp (ref R19)
      (value 510)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet https://www.seielect.com/Catalog/SEI-RMCF_RMCP.pdf)
      (fields
        (field (name Description) "RES 510 OHM 1% 1/8W 0805")
        (field (name "JEDEC Pkg") 0805)
        (field (name Manufacturer) "Stackpole Electronics Inc.")
        (field (name "Mfr PN") RMCF0805FT510R)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") RMCF0805FT510RCT-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=RMCF0805FT510RCT-ND))
      (libsource (lib proper-passives) (part R) (description ""))
      (sheetpath (names /rgb2component/) (tstamps /5A8FE7B6/))
      (tstamp 5A90453A))
    (comp (ref R20)
      (value 510)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet https://www.seielect.com/Catalog/SEI-RMCF_RMCP.pdf)
      (fields
        (field (name Description) "RES 510 OHM 1% 1/8W 0805")
        (field (name "JEDEC Pkg") 0805)
        (field (name Manufacturer) "Stackpole Electronics Inc.")
        (field (name "Mfr PN") RMCF0805FT510R)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") RMCF0805FT510RCT-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=RMCF0805FT510RCT-ND))
      (libsource (lib proper-passives) (part R) (description ""))
      (sheetpath (names /rgb2component/) (tstamps /5A8FE7B6/))
      (tstamp 5A9045DB))
    (comp (ref C16)
      (value 10u)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet http://www.samsungsem.com/kr/support/product-search/mlcc/CL21F106ZPFNNNE.jsp)
      (fields
        (field (name Description) "CAP CER 10UF 10V Y5V 0805")
        (field (name "JEDEC Pkg") 0805)
        (field (name Manufacturer) "Samsung Electro-Mechanics")
        (field (name "Mfr PN") CL21F106ZPFNNNE)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") 1276-3012-1-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=1276-3012-1-ND))
      (libsource (lib proper-passives) (part C) (description ""))
      (sheetpath (names /rgb2component/) (tstamps /5A8FE7B6/))
      (tstamp 5A904E08))
    (comp (ref C17)
      (value 10u)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet http://www.samsungsem.com/kr/support/product-search/mlcc/CL21F106ZPFNNNE.jsp)
      (fields
        (field (name Description) "CAP CER 10UF 10V Y5V 0805")
        (field (name "JEDEC Pkg") 0805)
        (field (name Manufacturer) "Samsung Electro-Mechanics")
        (field (name "Mfr PN") CL21F106ZPFNNNE)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") 1276-3012-1-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=1276-3012-1-ND))
      (libsource (lib proper-passives) (part C) (description ""))
      (sheetpath (names /rgb2component/) (tstamps /5A8FE7B6/))
      (tstamp 5A905259))
    (comp (ref C15)
      (value 0.1u)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet http://www.samsungsem.com/kr/support/product-search/mlcc/CL21F104ZBCNNNC.jsp)
      (fields
        (field (name Description) "CAP CER 0.1UF 50V Y5V 0805")
        (field (name "JEDEC Pkg") 0805)
        (field (name Manufacturer) "Samsung Electro-Mechanics")
        (field (name "Mfr PN") CL21F104ZBCNNNC)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") 1276-1007-1-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=1276-1007-1-ND))
      (libsource (lib proper-passives) (part C) (description ""))
      (sheetpath (names /rgb2component/) (tstamps /5A8FE7B6/))
      (tstamp 5A9052CB))
    (comp (ref R24)
      (value 75)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet https://www.seielect.com/Catalog/SEI-RMCF_RMCP.pdf)
      (fields
        (field (name Description) "RES 75 OHM 1% 1/8W 0805")
        (field (name "JEDEC Pkg") 0805)
        (field (name Manufacturer) "Stackpole Electronics Inc.")
        (field (name "Mfr PN") RMCF0805FT75R0)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") RMCF0805FT75R0CT-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=RMCF0805FT75R0CT-ND))
      (libsource (lib proper-passives) (part R) (description ""))
      (sheetpath (names /rgb2component/) (tstamps /5A8FE7B6/))
      (tstamp 5A905FEE))
    (comp (ref R25)
      (value 75)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet https://www.seielect.com/Catalog/SEI-RMCF_RMCP.pdf)
      (fields
        (field (name Description) "RES 75 OHM 1% 1/8W 0805")
        (field (name "JEDEC Pkg") 0805)
        (field (name Manufacturer) "Stackpole Electronics Inc.")
        (field (name "Mfr PN") RMCF0805FT75R0)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") RMCF0805FT75R0CT-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=RMCF0805FT75R0CT-ND))
      (libsource (lib proper-passives) (part R) (description ""))
      (sheetpath (names /rgb2component/) (tstamps /5A8FE7B6/))
      (tstamp 5A90613E))
    (comp (ref R23)
      (value 75)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet https://www.seielect.com/Catalog/SEI-RMCF_RMCP.pdf)
      (fields
        (field (name Description) "RES 75 OHM 1% 1/8W 0805")
        (field (name "JEDEC Pkg") 0805)
        (field (name Manufacturer) "Stackpole Electronics Inc.")
        (field (name "Mfr PN") RMCF0805FT75R0)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") RMCF0805FT75R0CT-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=RMCF0805FT75R0CT-ND))
      (libsource (lib proper-passives) (part R) (description ""))
      (sheetpath (names /rgb2component/) (tstamps /5A8FE7B6/))
      (tstamp 5A9061D5))
    (comp (ref J4)
      (value Triple_Coax)
      (footprint conns:triple-coax)
      (fields
        (field (name Note) "footprint is for a part obtained from a random AliExpress seller; can probably substitute one each of CUI RCJ-042/045/046")
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y))
      (libsource (lib triple_coax) (part Triple_Coax) (description "triple coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, ...)"))
      (sheetpath (names /rgb2component/) (tstamps /5A8FE7B6/))
      (tstamp 5A903F9F))
    (comp (ref U13)
      (value 74HCT04)
      (footprint Housings_SOIC:SOIC-14_3.9x8.7mm_Pitch1.27mm)
      (datasheet https://assets.nexperia.com/documents/data-sheet/74HC_HCT04.pdf)
      (fields
        (field (name Description) "IC INVERTER 6CH 6-INP 14SO")
        (field (name "JEDEC Pkg") SOIC-14)
        (field (name Manufacturer) "Nexperia USA Inc.")
        (field (name "Mfr PN") 74HCT04D,652)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") 1727-3798-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=1727-3798-ND))
      (libsource (lib rgb2svid-rescue) (part 74HCT04) (description ""))
      (sheetpath (names /oscillator/) (tstamps /5A932E50/))
      (tstamp 5A933EA8))
    (comp (ref Y1)
      (value "3.579545 MHz")
      (footprint Crystal:Crystal_SMD_HC49-SD)
      (datasheet http://www.foxonline.com/pdfs/C4SD.pdf)
      (fields
        (field (name Description) "CRYSTAL 3.579545MHZ 18PF SMD")
        (field (name "JEDEC Pkg") HC-49/US)
        (field (name Manufacturer) "Fox Electronics")
        (field (name "Mfr PN") FC4SDCBLF3.579545-T1)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") 631-1003-2-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=631-1003-2-ND))
      (libsource (lib Device) (part Crystal) (description "Two pin crystal"))
      (sheetpath (names /oscillator/) (tstamps /5A932E50/))
      (tstamp 5A9343E1))
    (comp (ref R26)
      (value 4.7M)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet https://www.seielect.com/Catalog/SEI-RMCF_RMCP.pdf)
      (fields
        (field (name Description) "RES 4.7M OHM 1% 1/8W 0805")
        (field (name "JEDEC Pkg") 0805)
        (field (name Manufacturer) "Stackpole Electronics Inc.")
        (field (name "Mfr PN") RMCF0805FT4M70)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") RMCF0805FT4M70CT-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=RMCF0805FT4M70CT-ND))
      (libsource (lib proper-passives) (part R) (description ""))
      (sheetpath (names /oscillator/) (tstamps /5A932E50/))
      (tstamp 5A93457D))
    (comp (ref C18)
      (value 33p)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet http://www.samsungsem.com/kr/support/product-search/mlcc/CL21C330JBANNNC.jsp)
      (fields
        (field (name Description) "CAP CER 33PF 50V C0G/NP0 0805")
        (field (name "JEDEC Pkg") 0805)
        (field (name Manufacturer) "Samsung Electro-Mechanics")
        (field (name "Mfr PN") CL21C330JBANNNC)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") 1276-1105-1-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=1276-1105-1-ND))
      (libsource (lib proper-passives) (part C) (description ""))
      (sheetpath (names /oscillator/) (tstamps /5A932E50/))
      (tstamp 5A934605))
    (comp (ref C19)
      (value 33p)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet http://www.samsungsem.com/kr/support/product-search/mlcc/CL21C330JBANNNC.jsp)
      (fields
        (field (name Description) "CAP CER 33PF 50V C0G/NP0 0805")
        (field (name "JEDEC Pkg") 0805)
        (field (name Manufacturer) "Samsung Electro-Mechanics")
        (field (name "Mfr PN") CL21C330JBANNNC)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") 1276-1105-1-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=1276-1105-1-ND))
      (libsource (lib proper-passives) (part C) (description ""))
      (sheetpath (names /oscillator/) (tstamps /5A932E50/))
      (tstamp 5A93472B))
    (comp (ref C20)
      (value 0.1u)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet http://www.samsungsem.com/kr/support/product-search/mlcc/CL21F104ZBCNNNC.jsp)
      (fields
        (field (name Description) "CAP CER 0.1UF 50V Y5V 0805")
        (field (name "JEDEC Pkg") 0805)
        (field (name Manufacturer) "Samsung Electro-Mechanics")
        (field (name "Mfr PN") CL21F104ZBCNNNC)
        (field (name "Qty Per Unit") 1)
        (field (name "Subs OK?") y)
        (field (name "Vendor 1 PN") 1276-1007-1-ND)
        (field (name "Vendor 1 URL") https://www.digikey.com/products/en?keywords=1276-1007-1-ND))
      (libsource (lib proper-passives) (part C) (description ""))
      (sheetpath (names /oscillator/) (tstamps /5A932E50/))
      (tstamp 5A935263)))
  (libparts
    (libpart (lib Device) (part Crystal)
      (description "Two pin crystal")
      (docs ~)
      (footprints
        (fp Crystal*))
      (fields
        (field (name Reference) Y)
        (field (name Value) Crystal))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib Device) (part Jumper_NC_Small)
      (description "Jumper, normally closed")
      (docs ~)
      (fields
        (field (name Reference) JP)
        (field (name Value) Jumper_NC_Small))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib Device) (part Jumper_NO_Small)
      (description "Jumper, normally open")
      (docs ~)
      (fields
        (field (name Reference) JP)
        (field (name Value) Jumper_NO_Small))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib apple2) (part IIGS_RGB)
      (description "Apple IIGS RGB output")
      (docs http://apple2.info/wiki/index.php?title=Pinouts#IIGS_.28and_Apple_.2F.2F.2F.29_RGB_Connector)
      (footprints
        (fp DSUB-15_Male))
      (fields
        (field (name Reference) J)
        (field (name Value) IIGS_RGB))
      (pins
        (pin (num 1) (name GND) (type passive))
        (pin (num 2) (name RED) (type passive))
        (pin (num 3) (name CSYNC) (type passive))
        (pin (num 4) (name NC) (type NotConnected))
        (pin (num 5) (name GREEN) (type passive))
        (pin (num 6) (name GND) (type passive))
        (pin (num 7) (name -5V) (type passive))
        (pin (num 8) (name +12V) (type passive))
        (pin (num 9) (name BLUE) (type passive))
        (pin (num 10) (name NC) (type NotConnected))
        (pin (num 11) (name SOUND) (type passive))
        (pin (num 12) (name NTSC/PAL) (type passive))
        (pin (num 13) (name GND) (type passive))
        (pin (num 14) (name NC) (type NotConnected))
        (pin (num 15) (name NC) (type NotConnected))))
    (libpart (lib cxa1645) (part CXA2075)
      (description "RGB to NTSC/PAL encoder")
      (docs http://pdf1.alldatasheet.com/datasheet-pdf/view/146350/SONY/CXA2075M/+0_5473VPMMZb.a.NBEDU+/datasheet.pdf)
      (footprints
        (fp sop:SOP-24_15.0x5.3mm_P1.27mm))
      (fields
        (field (name Reference) U)
        (field (name Value) CXA2075))
      (pins
        (pin (num 1) (name GND1) (type power_in))
        (pin (num 2) (name RIN) (type input))
        (pin (num 3) (name GIN) (type input))
        (pin (num 4) (name BIN) (type input))
        (pin (num 5) (name NC) (type NotConnected))
        (pin (num 6) (name SCIN) (type input))
        (pin (num 7) (name NPIN) (type input))
        (pin (num 8) (name BFOUT) (type output))
        (pin (num 9) (name NC) (type NotConnected))
        (pin (num 10) (name SYNCIN) (type input))
        (pin (num 11) (name NC) (type NotConnected))
        (pin (num 12) (name VCC1) (type power_in))
        (pin (num 13) (name NC) (type NotConnected))
        (pin (num 14) (name NC) (type NotConnected))
        (pin (num 15) (name COUT) (type output))
        (pin (num 16) (name YOUT) (type output))
        (pin (num 17) (name YTRAP) (type input))
        (pin (num 18) (name NC) (type NotConnected))
        (pin (num 19) (name VCC2) (type power_in))
        (pin (num 20) (name CVOUT) (type output))
        (pin (num 21) (name BOUT) (type output))
        (pin (num 22) (name GOUT) (type output))
        (pin (num 23) (name ROUT) (type output))
        (pin (num 24) (name GND2) (type power_in))))
    (libpart (lib proper-passives) (part C)
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib proper-passives) (part CP)
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib proper-passives) (part R)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib rgb2svid-rescue) (part 74HCT04)
      (fields
        (field (name Reference) U)
        (field (name Value) 74HCT04))
      (pins
        (pin (num 1) (name ~) (type input))
        (pin (num 2) (name ~) (type output))
        (pin (num 3) (name ~) (type input))
        (pin (num 4) (name ~) (type output))
        (pin (num 5) (name ~) (type input))
        (pin (num 6) (name ~) (type output))
        (pin (num 7) (name GND) (type power_in))
        (pin (num 8) (name ~) (type output))
        (pin (num 9) (name ~) (type input))
        (pin (num 10) (name ~) (type output))
        (pin (num 11) (name ~) (type input))
        (pin (num 12) (name ~) (type output))
        (pin (num 13) (name ~) (type input))
        (pin (num 14) (name VCC) (type power_in))))
    (libpart (lib rgb2svid-rescue) (part Conn_Coaxial)
      (footprints
        (fp *BNC*)
        (fp *SMA*)
        (fp *SMB*)
        (fp *SMC*)
        (fp *Cinch*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_Coaxial))
      (pins
        (pin (num 1) (name In) (type passive))
        (pin (num 2) (name Ext) (type passive))))
    (libpart (lib rgb2svid-rescue) (part L7805)
      (footprints
        (fp TO?252*)
        (fp TO?263*)
        (fp TO?220*))
      (fields
        (field (name Reference) U)
        (field (name Value) L7805))
      (pins
        (pin (num 1) (name IN) (type power_in))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name OUT) (type power_out))))
    (libpart (lib rgb2svid-rescue) (part MC33079)
      (footprints
        (fp SOIC*3.9x8.7mm*Pitch1.27mm*)
        (fp DIP*W7.62mm*)
        (fp TSSOP*4.4x5mm*Pitch0.65mm*)
        (fp SSOP*5.3x6.2mm*Pitch0.65mm*)
        (fp MSOP*3x3mm*Pitch0.5mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) MC33079))
      (pins
        (pin (num 1) (name ~) (type output))
        (pin (num 2) (name -) (type input))
        (pin (num 3) (name +) (type input))
        (pin (num 4) (name V+) (type power_in))
        (pin (num 5) (name +) (type input))
        (pin (num 6) (name -) (type input))
        (pin (num 7) (name ~) (type output))
        (pin (num 8) (name ~) (type output))
        (pin (num 9) (name -) (type input))
        (pin (num 10) (name +) (type input))
        (pin (num 11) (name V-) (type power_in))
        (pin (num 12) (name +) (type input))
        (pin (num 13) (name -) (type input))
        (pin (num 14) (name ~) (type output))))
    (libpart (lib rgb2svid-rescue) (part Mini-DIN-4)
      (footprints
        (fp MINI?DIN*))
      (fields
        (field (name Reference) J)
        (field (name Value) Mini-DIN-4))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))))
    (libpart (lib triple_coax) (part Triple_Coax)
      (description "triple coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, ...)")
      (footprints
        (fp *BNC*)
        (fp *SMA*)
        (fp *SMB*)
        (fp *SMC*)
        (fp *Cinch*))
      (fields
        (field (name Reference) J)
        (field (name Value) Triple_Coax))
      (pins
        (pin (num 1) (name In) (type passive))
        (pin (num 2) (name Ext) (type passive))
        (pin (num 3) (name In) (type passive))
        (pin (num 4) (name Ext) (type passive))
        (pin (num 5) (name In) (type passive))
        (pin (num 6) (name Ext) (type passive))))
    (libpart (lib via) (part via)
      (fields
        (field (name Reference) U)
        (field (name Value) via))
      (pins
        (pin (num 1) (name ~) (type input)))))
  (libraries
    (library (logical Device)
      (uri /usr/share/kicad/symbols/Device.lib))
    (library (logical apple2)
      (uri /root/rgb2svid/kicad-libs/apple2.lib))
    (library (logical cxa1645)
      (uri /root/rgb2svid/kicad-libs/cxa1645.lib))
    (library (logical proper-passives)
      (uri /root/rgb2svid/kicad-libs/proper-passives.lib))
    (library (logical rgb2svid-rescue)
      (uri /root/rgb2svid/rgb2svid-rescue.lib))
    (library (logical triple_coax)
      (uri /root/rgb2svid/kicad-libs/triple_coax.lib))
    (library (logical via)
      (uri /root/rgb2svid/kicad-libs/via.lib)))
  (nets
    (net (code 1) (name "Net-(J1-Pad12)")
      (node (ref J1) (pin 12)))
    (net (code 2) (name "Net-(J1-Pad11)")
      (node (ref J1) (pin 11)))
    (net (code 3) (name "Net-(U2-Pad8)")
      (node (ref U2) (pin 8)))
    (net (code 4) (name GND)
      (node (ref C7) (pin 2))
      (node (ref J1) (pin 6))
      (node (ref J1) (pin 13))
      (node (ref C3) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref U1) (pin 2))
      (node (ref U2) (pin 1))
      (node (ref J3) (pin 1))
      (node (ref J3) (pin 2))
      (node (ref U2) (pin 24))
      (node (ref C6) (pin 2))
      (node (ref C9) (pin 2))
      (node (ref C8) (pin 2))
      (node (ref U13) (pin 7))
      (node (ref U13) (pin 7))
      (node (ref U13) (pin 3))
      (node (ref U13) (pin 7))
      (node (ref C20) (pin 2))
      (node (ref C18) (pin 2))
      (node (ref C19) (pin 1))
      (node (ref U13) (pin 11))
      (node (ref U13) (pin 5))
      (node (ref U13) (pin 7))
      (node (ref U13) (pin 9))
      (node (ref U13) (pin 7))
      (node (ref U13) (pin 7))
      (node (ref R7) (pin 1))
      (node (ref J4) (pin 2))
      (node (ref R6) (pin 1))
      (node (ref R8) (pin 1))
      (node (ref J4) (pin 4))
      (node (ref C14) (pin 2))
      (node (ref U3) (pin 3))
      (node (ref U3) (pin 5))
      (node (ref R22) (pin 1))
      (node (ref C16) (pin 2))
      (node (ref C17) (pin 1))
      (node (ref C15) (pin 1))
      (node (ref R20) (pin 1))
      (node (ref J4) (pin 6))
      (node (ref U9) (pin 1))
      (node (ref JP2) (pin 1))
      (node (ref U8) (pin 1))
      (node (ref U11) (pin 1))
      (node (ref U12) (pin 1))
      (node (ref J2) (pin 2))
      (node (ref U10) (pin 1))
      (node (ref U6) (pin 1))
      (node (ref U7) (pin 1))
      (node (ref J1) (pin 1))
      (node (ref U5) (pin 1))
      (node (ref U4) (pin 1)))
    (net (code 5) (name "Net-(C10-Pad1)")
      (node (ref R2) (pin 2))
      (node (ref C10) (pin 1)))
    (net (code 6) (name "Net-(R2-Pad1)")
      (node (ref R2) (pin 1))
      (node (ref U2) (pin 20)))
    (net (code 7) (name "Net-(C10-Pad2)")
      (node (ref J2) (pin 1))
      (node (ref C10) (pin 2)))
    (net (code 8) (name VEE)
      (node (ref U3) (pin 11))
      (node (ref U3) (pin 11))
      (node (ref U3) (pin 11))
      (node (ref C17) (pin 2))
      (node (ref C15) (pin 2))
      (node (ref J1) (pin 7))
      (node (ref U3) (pin 11)))
    (net (code 9) (name /B_OUT)
      (node (ref U19) (pin 1))
      (node (ref R13) (pin 1))
      (node (ref R8) (pin 2))
      (node (ref R11) (pin 1))
      (node (ref U2) (pin 21)))
    (net (code 10) (name /G_OUT)
      (node (ref U18) (pin 1))
      (node (ref U2) (pin 22))
      (node (ref R5) (pin 1)))
    (net (code 11) (name /R_OUT)
      (node (ref U2) (pin 23))
      (node (ref R12) (pin 1))
      (node (ref U17) (pin 1))
      (node (ref R10) (pin 2))
      (node (ref R6) (pin 2)))
    (net (code 12) (name /B_IN)
      (node (ref U2) (pin 4))
      (node (ref U16) (pin 1))
      (node (ref C5) (pin 2)))
    (net (code 13) (name /G_IN)
      (node (ref U2) (pin 3))
      (node (ref U15) (pin 1))
      (node (ref C4) (pin 2)))
    (net (code 14) (name /R_IN)
      (node (ref U14) (pin 1))
      (node (ref U2) (pin 2))
      (node (ref C2) (pin 2)))
    (net (code 15) (name "Net-(JP1-Pad2)")
      (node (ref JP1) (pin 2))
      (node (ref JP2) (pin 2))
      (node (ref U2) (pin 7)))
    (net (code 16) (name /+12V)
      (node (ref U1) (pin 1))
      (node (ref C1) (pin 1))
      (node (ref J1) (pin 8)))
    (net (code 17) (name /oscillator/XOUT)
      (node (ref U13) (pin 12))
      (node (ref U2) (pin 6)))
    (net (code 18) (name VCC)
      (node (ref C6) (pin 1))
      (node (ref C7) (pin 1))
      (node (ref U1) (pin 3))
      (node (ref C3) (pin 1))
      (node (ref U2) (pin 12))
      (node (ref U2) (pin 19))
      (node (ref C14) (pin 1))
      (node (ref U3) (pin 4))
      (node (ref U3) (pin 4))
      (node (ref U3) (pin 4))
      (node (ref U13) (pin 14))
      (node (ref U3) (pin 4))
      (node (ref C9) (pin 1))
      (node (ref C8) (pin 1))
      (node (ref U13) (pin 14))
      (node (ref JP1) (pin 1))
      (node (ref C20) (pin 1))
      (node (ref R1) (pin 1))
      (node (ref U13) (pin 14))
      (node (ref U13) (pin 14))
      (node (ref U13) (pin 14))
      (node (ref U13) (pin 14))
      (node (ref C16) (pin 1)))
    (net (code 19) (name "Net-(C2-Pad1)")
      (node (ref C2) (pin 1))
      (node (ref J1) (pin 2)))
    (net (code 20) (name /rgb2component/Sync)
      (node (ref U2) (pin 10))
      (node (ref J1) (pin 3))
      (node (ref C13) (pin 2)))
    (net (code 21) (name "Net-(C5-Pad1)")
      (node (ref C5) (pin 1))
      (node (ref J1) (pin 9)))
    (net (code 22) (name "Net-(C4-Pad1)")
      (node (ref J1) (pin 5))
      (node (ref C4) (pin 1)))
    (net (code 23) (name "Net-(R1-Pad2)")
      (node (ref U2) (pin 17))
      (node (ref R1) (pin 2)))
    (net (code 24) (name "Net-(C11-Pad2)")
      (node (ref C11) (pin 2))
      (node (ref J3) (pin 3)))
    (net (code 25) (name "Net-(R3-Pad1)")
      (node (ref U2) (pin 16))
      (node (ref R3) (pin 1)))
    (net (code 26) (name "Net-(C12-Pad1)")
      (node (ref R4) (pin 2))
      (node (ref C12) (pin 1)))
    (net (code 27) (name "Net-(R4-Pad1)")
      (node (ref U2) (pin 15))
      (node (ref R4) (pin 1)))
    (net (code 28) (name "Net-(C11-Pad1)")
      (node (ref C11) (pin 1))
      (node (ref R3) (pin 2)))
    (net (code 29) (name "Net-(J1-Pad15)")
      (node (ref J1) (pin 15)))
    (net (code 30) (name "Net-(J1-Pad14)")
      (node (ref J1) (pin 14)))
    (net (code 31) (name "Net-(J1-Pad10)")
      (node (ref J1) (pin 10)))
    (net (code 32) (name "Net-(J1-Pad4)")
      (node (ref J1) (pin 4)))
    (net (code 33) (name "Net-(U2-Pad11)")
      (node (ref U2) (pin 11)))
    (net (code 34) (name "Net-(U2-Pad9)")
      (node (ref U2) (pin 9)))
    (net (code 35) (name "Net-(U2-Pad13)")
      (node (ref U2) (pin 13)))
    (net (code 36) (name "Net-(U2-Pad5)")
      (node (ref U2) (pin 5)))
    (net (code 37) (name "Net-(C12-Pad2)")
      (node (ref C12) (pin 2))
      (node (ref J3) (pin 4)))
    (net (code 38) (name "Net-(U2-Pad18)")
      (node (ref U2) (pin 18)))
    (net (code 39) (name "Net-(U2-Pad14)")
      (node (ref U2) (pin 14)))
    (net (code 40) (name "Net-(R19-Pad1)")
      (node (ref R19) (pin 1))
      (node (ref R20) (pin 2))
      (node (ref U3) (pin 9)))
    (net (code 41) (name "Net-(R19-Pad2)")
      (node (ref U3) (pin 8))
      (node (ref R19) (pin 2))
      (node (ref R23) (pin 1)))
    (net (code 42) (name "Net-(R21-Pad1)")
      (node (ref U3) (pin 13))
      (node (ref R22) (pin 2))
      (node (ref R21) (pin 1)))
    (net (code 43) (name "Net-(R21-Pad2)")
      (node (ref U3) (pin 14))
      (node (ref R21) (pin 2))
      (node (ref R24) (pin 1)))
    (net (code 44) (name "Net-(R17-Pad2)")
      (node (ref U3) (pin 6))
      (node (ref R18) (pin 2))
      (node (ref R17) (pin 2)))
    (net (code 45) (name "Net-(R18-Pad1)")
      (node (ref R25) (pin 1))
      (node (ref U3) (pin 7))
      (node (ref R18) (pin 1)))
    (net (code 46) (name "Net-(R13-Pad2)")
      (node (ref R16) (pin 1))
      (node (ref R13) (pin 2))
      (node (ref U3) (pin 10)))
    (net (code 47) (name "Net-(R12-Pad2)")
      (node (ref R15) (pin 2))
      (node (ref R12) (pin 2))
      (node (ref U3) (pin 12)))
    (net (code 48) (name "Net-(C13-Pad1)")
      (node (ref R5) (pin 2))
      (node (ref R9) (pin 1))
      (node (ref C13) (pin 1))
      (node (ref R7) (pin 2)))
    (net (code 49) (name "Net-(R10-Pad1)")
      (node (ref R10) (pin 1))
      (node (ref R11) (pin 2))
      (node (ref R9) (pin 2))
      (node (ref U3) (pin 2))
      (node (ref R14) (pin 2)))
    (net (code 50) (name "Net-(R14-Pad1)")
      (node (ref R16) (pin 2))
      (node (ref R17) (pin 1))
      (node (ref R14) (pin 1))
      (node (ref U3) (pin 1))
      (node (ref R15) (pin 1)))
    (net (code 51) (name "Net-(J4-Pad3)")
      (node (ref R23) (pin 2))
      (node (ref J4) (pin 3)))
    (net (code 52) (name "Net-(J4-Pad1)")
      (node (ref R25) (pin 2))
      (node (ref J4) (pin 1)))
    (net (code 53) (name "Net-(J4-Pad5)")
      (node (ref R24) (pin 2))
      (node (ref J4) (pin 5)))
    (net (code 54) (name "Net-(C19-Pad2)")
      (node (ref C19) (pin 2))
      (node (ref R26) (pin 2))
      (node (ref U13) (pin 2))
      (node (ref Y1) (pin 2))
      (node (ref U13) (pin 13)))
    (net (code 55) (name "Net-(C18-Pad1)")
      (node (ref C18) (pin 1))
      (node (ref Y1) (pin 1))
      (node (ref U13) (pin 1))
      (node (ref R26) (pin 1)))
    (net (code 56) (name "Net-(U13-Pad10)")
      (node (ref U13) (pin 10)))
    (net (code 57) (name "Net-(U13-Pad8)")
      (node (ref U13) (pin 8)))
    (net (code 58) (name "Net-(U13-Pad6)")
      (node (ref U13) (pin 6)))
    (net (code 59) (name "Net-(U13-Pad4)")
      (node (ref U13) (pin 4)))))