(footprint "Heatsink_56x56mm_2xFixation3.2mm" (version 20210228) (generator pcbnew) (layer "F.Cu")
  (tedit 60B235E1)
  (descr "Heatsink, 56 x 56mm, 2x 3.2mm Drills,")
  (tags "heatsink")
  (attr through_hole)
  (fp_text reference "REF**" (at -28.1 -31.2) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp d27c1f77-06fe-4340-a1db-4cedf16d9abf)
  )
  (fp_text value "Heatsink_56x56mm_2xFixation3.2mm" (at 0 31) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c9b8ea0a-b058-428a-8f4b-e265682abc48)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 17413c1b-3962-412c-ad14-1b74a6277762)
  )
  (fp_circle (center 25 -25) (end 28.2 -25) (layer "Cmts.User") (width 0.15) (fill none) (tstamp 2ea97b72-f1c5-4934-acd6-38fabe42c1cb))
  (fp_circle (center -25 25) (end -21.8 25) (layer "Cmts.User") (width 0.15) (fill none) (tstamp 6a66e4b3-0ea6-470a-880d-8e8cd43635dc))
  (fp_circle (center -25 25) (end -21.55 25) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp 648f4d43-f2da-4ebe-b7e9-64311d322322))
  (fp_circle (center 25 -25) (end 28.45 -25) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp b88b718d-0ebc-4f09-8b07-5b30f829ec8c))
  (fp_line (start 28 -28) (end -28 -28) (layer "F.Fab") (width 0.1) (tstamp 2469f466-3de0-418d-8405-8f6caae389ce))
  (fp_line (start 28 -28) (end 28 28) (layer "F.Fab") (width 0.1) (tstamp 84a84cd4-6cb3-4afe-85ed-2270e26659c4))
  (fp_line (start 28 28) (end -28 28) (layer "F.Fab") (width 0.1) (tstamp e8ea5143-3763-4b66-8ad2-e5fed8f2afb8))
  (fp_line (start -28 -28) (end -28 28) (layer "F.Fab") (width 0.1) (tstamp e9b052ef-6275-4534-b1d4-3434f99706fa))
  (pad "" np_thru_hole circle (at -25 25) (locked) (size 3.2 3.2) (drill 3.2) (layers F&B.Cu *.Mask) (tstamp 72e5da35-e202-466d-8d9d-c09f3e19e15f))
  (pad "" np_thru_hole circle (at 25 -25) (locked) (size 3.2 3.2) (drill 3.2) (layers F&B.Cu *.Mask) (tstamp d54c55b6-a6c9-451b-8c99-0be0b8be4bde))
  (model "${KIPRJMOD}/Amber.3dshapes/Heatsink_56x56mm_2xFixation3.2mm.wrl"
    (offset (xyz 30 30 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 90))
  )
)
