(footprint "Heatsink_60x60mm_2xFixation3.2mm" (version 20210108) (generator pcbnew) (layer "F.Cu")
  (tedit 6022E2BF)
  (descr "Heatsink, 60 x 60mm, 2x 3.2mm Drills,")
  (tags "heatsink")
  (attr through_hole)
  (fp_text reference "REF**" (at 1.9 -1.2) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp d27c1f77-06fe-4340-a1db-4cedf16d9abf)
  )
  (fp_text value "Heatsink_60x60mm_2xFixation3.2mm" (at 30 61) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c9b8ea0a-b058-428a-8f4b-e265682abc48)
  )
  (fp_text user "${REFERENCE}" (at 30 30) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 17413c1b-3962-412c-ad14-1b74a6277762)
  )
  (fp_line (start -0.1 5.1) (end -0.1 -0.1) (layer "F.SilkS") (width 0.12) (tstamp 084b3e0a-0d4d-4957-8b8a-5655892eafd8))
  (fp_line (start 60.1 60.1) (end 55.1 60.1) (layer "F.SilkS") (width 0.12) (tstamp 0c9248af-c23f-4b5b-ad46-186a6cfca0d2))
  (fp_line (start 5.1 60.1) (end -0.1 60.1) (layer "F.SilkS") (width 0.12) (tstamp 689b56fd-d0f5-42e9-a7dc-aaccdde90e38))
  (fp_line (start 55.1 -0.1) (end 60.1 -0.1) (layer "F.SilkS") (width 0.12) (tstamp 842bbc34-bcfd-4aa7-8f73-bd41bc9a051f))
  (fp_line (start -0.1 -0.1) (end 5.1 -0.1) (layer "F.SilkS") (width 0.12) (tstamp 8b56ba46-dc87-4c16-b40d-833aea901c19))
  (fp_line (start 60.1 5.1) (end 60.1 -0.1) (layer "F.SilkS") (width 0.12) (tstamp ae0bb233-a7cd-46f6-8df0-a663a3a5035b))
  (fp_line (start -0.1 60.1) (end -0.1 55.1) (layer "F.SilkS") (width 0.12) (tstamp b3baace2-ddc4-4152-99d7-acfc6abdf917))
  (fp_line (start 60.1 60.1) (end 60.1 55.1) (layer "F.SilkS") (width 0.12) (tstamp c98f8d9c-105b-412b-8a21-03d9d2160187))
  (fp_circle (center 55 55) (end 58.2 55) (layer "Cmts.User") (width 0.15) (fill none) (tstamp 2ea97b72-f1c5-4934-acd6-38fabe42c1cb))
  (fp_circle (center 5 5) (end 8.2 5) (layer "Cmts.User") (width 0.15) (fill none) (tstamp 6a66e4b3-0ea6-470a-880d-8e8cd43635dc))
  (fp_circle (center 5 5) (end 8.45 5) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp 648f4d43-f2da-4ebe-b7e9-64311d322322))
  (fp_circle (center 55 55) (end 58.45 55) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp b88b718d-0ebc-4f09-8b07-5b30f829ec8c))
  (fp_line (start 60 0) (end 0 0) (layer "F.Fab") (width 0.1) (tstamp 2469f466-3de0-418d-8405-8f6caae389ce))
  (fp_line (start 60 0) (end 60 60) (layer "F.Fab") (width 0.1) (tstamp 84a84cd4-6cb3-4afe-85ed-2270e26659c4))
  (fp_line (start 60 60) (end 0 60) (layer "F.Fab") (width 0.1) (tstamp e8ea5143-3763-4b66-8ad2-e5fed8f2afb8))
  (fp_line (start 0 0) (end 0 60) (layer "F.Fab") (width 0.1) (tstamp e9b052ef-6275-4534-b1d4-3434f99706fa))
  (pad "" np_thru_hole circle (at 5 5) (locked) (size 3.2 3.2) (drill 3.2) (layers F&B.Cu *.Mask) (tstamp 72e5da35-e202-466d-8d9d-c09f3e19e15f))
  (pad "" np_thru_hole circle (at 55 55) (locked) (size 3.2 3.2) (drill 3.2) (layers F&B.Cu *.Mask) (tstamp d54c55b6-a6c9-451b-8c99-0be0b8be4bde))
  (model "${KISYS3DMOD}/Heatsink.3dshapes/Heatsink_62x40mm_2xFixation3mm.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
